For 1990-2009 cars

Callout | Component Name
--- | ---
Front Side Marker Lamp Replacement Preliminary Procedure Remove the front fascia extension to gain access to the front side marker lamp. Refer to Fascia, Extension, Reinforcement and Impact Bar Replacement - Front Bumper in Bumpers.
1 | Front Side Marker Lamp Assembly Replacement Tip

• | Release the tab from the inside of the panel, and push outward to replace the lamp assembly.

• | Rotate the lamp socket, pull inward to replace the bulb.