For 1990-2009 cars

### Removal Procedure

1. Remove the air conditioning, power steering and water pump drive belt. Refer to Water Pump and Air Conditioning Compressor and Power Steering Pump Belt Replacement.
2. Remove the drive belt idler pulley bolt.
3. Remove the drive belt idler pulley.

### Installation Procedure

1. Install the drive belt idler pulley.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the drive belt idler pulley bolt.

Tighten
Tighten the drive belt idler pulley bolt to 50 N·m (37 lb ft).

3. Install the drive belt. Refer to Water Pump and Air Conditioning Compressor and Power Steering Pump Belt Replacement.