For 1990-2009 cars

### Removal Procedure

1. Disconnect the ambient air temperature sensor electrical connector (1).
2. Release the ambient air temperature sensor from the clip.
3. Remove the ambient air temperature sensor from the vehicle.

### Installation Procedure

1. Place the ambient air temperature sensor in position.
2. Engage the ambient air temperature sensor into the clip.
3. Connect the ambient air temperature electrical connector (1).