For 1990-2009 cars

Callout | Component Name
--- | ---

#### Rear Side Door Assembly Replacement

1 | Rear Side Door Hinge Lower Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 25 N·m (18 lb ft)
2 | Rear Side Door Hinge Upper Bolt (Qty: 2) Tighten 25 N·m (18 lb ft)
3 | Rear Side Door Assembly Tip Disconnect the rear door wiring harness connector and reconnect when finished with replacement.

#### Rear Side Door Lower Hinge Assembly Replacement

Tip
Replace only one hinge at a time.

1 | Rear Side Door Hinge Lower Bolt (Qty: 2) Tighten 25 N·m (18 lb ft)
4 | Rear Side Door Hinge Lower Bolt (Qty: 2) Tighten 25 N·m (18 lb ft)
5 | Rear Side Door Lower Hinge Assembly Replacement

#### Rear Side Door Upper Hinge Assembly Replacement

Tip
Replace only one hinge at a time.

2 | Rear Side Door Hinge Upper Bolt (Qty: 2) Tighten 25 N·m (18 lb ft)
6 | Rear Side Door Hinge Upper Bolt (Qty: 2) Tighten 25 N·m (18 lb ft)
7 | Rear Side Door Upper Hinge Assembly