For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
Schematic Reference: Shift Lock Control Schematics Connector End View Reference: Shift Lock Control Connector End Views or 52096 DEFINITION: Transmission shift lever does not move out of the PARK position with the ignition ON and the brake pedal depressed.
1 | Did you perform the Diagnostic System Check - Vehicle? | Go to Step 2 | Go to Diagnostic System Check - Vehicle
2 |

1. Apply the parking brake and block the wheels.
2. Turn ON the ignition, with the engine OFF.
3. Attempt to move the shift lever out of the PARK position without pressing the brake pedal.

Does the shift lever move out of the PARK position?

Go to Testing for Intermittent Conditions and Poor Connections

Go to Step 3

3 |

1. Turn OFF the ignition.
2. Install a scan tool.
3. Turn ON the ignition, with the engine OFF.
4. Press and hold the brake pedal.
5. With a scan tool, observe the shift lock control output in the remote control door lock receiver (RCDLR) data list.

Does the scan tool display an Active status?

Go to Step 5

Go to Step 4

4 | With a scan tool, observe the brake switch input in the transmission control module (TCM) data list. Does the brake switch status indicate Active? | Go to Step 8 | Go to Stop Lamps Inoperative
5 |

1. Turn OFF the ignition.
2. Connect a test lamp at the shift lock control solenoid voltage supply circuit at the connector of the shift lock control solenoid and a good ground.
3. Turn ON the ignition, with the engine OFF.

Does the test lamp illuminate?

Go to Step 6

Go to Step 10

6 |

1. Turn OFF the ignition.
2. Disconnect the harness connector of the automatic transmission shift lock control solenoid.
3. Connect a test lamp between the shift lock control solenoid voltage supply circuit and the shift lock control solenoid control circuit at the connector of the shift lock control solenoid.
4. Turn ON the ignition, with the engine OFF.
5. With a scan tool, command the shift lock control output ON and OFF several times.

Does the test lamp turn ON and OFF with each command?

Go to Step 8

Go to Step 7

7 | Test the control circuit of the automatic transmission shift lock control solenoid for an open or short to voltage. Refer to Circuit Testing and Wiring Repairs. Did you find and correct the condition? | Go to Step 13 | Go to Step 9
8 | Inspect for poor connections at the harness connector of the automatic transmission shift lock control solenoid. Refer to Testing for Intermittent Conditions and Poor Connections and Connector Repairs. Did you find and correct the condition? | Go to Step 13 | Go to Step 11
9 | Inspect for poor connections at the harness connector of the RCDLR. Refer to Testing for Intermittent Conditions and Poor Connections and Connector Repairs. Did you find and correct the condition? | Go to Step 13 | Go to Step 12
10 | Repair the open or short to ground in the automatic transmission shift lock control solenoid voltage supply circuit. Refer to Circuit Testing and Wiring Repairs. Did you complete the repair? | Go to Step 13 | --
11 | Replace the automatic transmission shift lock control solenoid. Refer to Transmission Control Replacement. Did you complete the replacement? | Go to Step 13 | --
12 | Replace the RCDLR. Refer to Control Module References for replacement, setup, and programming. Did you complete the replacement? | Go to Step 13 | --
13 | Operate the system in order to verify the repair. Did you find and correct the condition? | System OK | Go to Step 2