For 1990-2009 cars

### Removal Procedure

1. Turn the ignition OFF.

Note: Do not disconnect the power steering fluid lines/hoses from the reservoir.

2. Remove the power steering fluid reservoir bolts and reposition the power steering fluid reservoir in order to provide access. Refer to Power Steering Fluid Reservoir Replacement.
3. Remove the camshaft position (CMP) actuator valve electrical connector.
4. Remove the camshaft position actuator valve bolts.
5. Remove the CMP actuator valve.
6. Inspect the CMP actuator valve seal for damage and replace as necessary.

### Installation Procedure

1. Inspect the CMP actuator valve seal for damage. Replace components if necessary.
2. Install the CMP actuator valve.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the CMP actuator valve bolt and tighten to 10 N·m (89 lb in).
4. Install the CMP actuator valve electrical connector.
5. Install the power steering fluid reservoir. Refer to Power Steering Fluid Reservoir Replacement.