For 1990-2009 cars

Callout | Component Name
--- | ---

#### Rear Bumper Fascia Replacement

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the rear wheelhouse liner panels. Refer to Rear Wheelhouse Panel Liner Replacement.

1 | Rear Bumper Fascia Screw Notice: Refer to Fastener Notice in the Preface section. Tip The screws are in the wheel opening. Tighten
3 N·m (27 lb in)

2 | Compartment Sill Trim Plate Assembly
3 | Rear Bumper Fascia Screw (Qty: 4) Tighten 6 N·m (53 lb in)
4 | Rear Bumper Fascia Retainer (Qty: 3) Tip Remove the retainer with inclined cutter, replace with new retainer while installing.
5 | Rear Bumper Fascia Assembly Tighten 6 N·m (5 lb in)