For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Air Cleaner Assembly Front Half Screws | 8 N·m | 71 lb in
Brake Line to Brake Hose Fitting | 27 N·m | 20 lb ft
Intermediate Steering Shaft Pinch Bolt | 48 N·m | 35 lb ft
Lower Engine Mount Nuts to Frame | 80 N·m | 59 lb ft
Outer Tie Rod to Knuckle Retaining Nut | 82 N·m | 60 lb ft
Power Steering Cooler Pipe/Hose to Frame Retaining Bolt | 10 N·m | 88 lb in
Power Steering Cooler to Bracket Retaining Bolts | 9 N·m | 80 lb in
Power Steering Gear Retaining Bolts
First Pass | 55 N·m | 40 lb ft
Second Pass | Retighten 80 Degrees
Power Steering Hoses to Power Steering Gear Retaining Bolt | 23 N·m | 17 lb ft
Power Steering Pressure Hose to Frame Retaining Bolts | 10 N·m | 88 lb in
Power Steering Pressure Hose to Power Steering Pump | 40 N·m | 30 lb ft
Power Steering Pump Bracket to Engine Bolt | 58 N·m | 43 lb ft
Power Steering Pump to Engine Bolt | 58 N·m | 43 lb ft
Power Steering Pump to Power Steering Bracket Bolt | 22 N·m | 16 lb ft
Power Steering Reservoir Retaining Nuts | 9 N·m | 80 lb in
Power Steering Return Line to Frame Retaining Bolt. | 10 N·m | 88 lb in