For 1990-2009 cars

### Removal Procedure

1. Remove the left intake camshaft actuator (6). Refer to Camshaft Position Actuator Replacement - Bank 2 (Left Side) Intake .
2. Remove the left exhaust camshaft actuator (9). Refer to Camshaft Position Actuator Replacement - Bank 2 (Left Side) Exhaust .
3. Remove the left intake camshaft. Refer to Intake Camshaft Removal - Left Side .
4. Remove the left exhaust camshaft. Refer to Exhaust Camshaft Removal - Left Side .
5. Clean and inspect the camshafts. Refer to Camshaft Cleaning and Inspection .

### Installation Procedure

1. Install the left exhaust camshaft. Refer to Exhaust Camshaft Installation - Left Side .
2. Install the left intake camshaft. Refer to Intake Camshaft Installation - Left Side .
3. Install the left exhaust camshaft actuator (9). Refer to Camshaft Position Actuator Replacement - Bank 2 (Left Side) Exhaust .
4. Install the left intake camshaft actuator (6). Refer to Camshaft Position Actuator Replacement - Bank 2 (Left Side) Intake .