For 1990-2009 cars

### Removal Procedure

1. Remove rear bumper fascia. Refer to Rear Bumper Fascia Replacement .
2. Disconnect electrical from the rear object sensor.
3. Lift the locking tabs on the housing and remove the rear object sensor.

### Installation Procedure

1. Put the rear object sensor downward in order to press it within the locking tabs on the housing.
2. Connect the sensor harness connector.
3. Install the bumper fascia.