For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel (I/P) center trim. Refer to Instrument Cluster Trim Panel Replacement .
2. Release the tabs securing the outlet air deflector to the I/P center trim.

### Installation Procedure

1. Locate the tabs securing the outlet air deflector to the I/P center trim.
2. Install the I/P center trim. Refer to Instrument Cluster Trim Panel Replacement .