For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the front air deflector. Refer to Front Air Deflector Replacement.
3. Disconnect the power steering cooler pipe/hose from the power steering lines.
4. Remove the power steering cooler pipe/hose to frame retaining bolt.
5. Lower the vehicle.
6. Disconnect the power steering cooler pipe/hose from the power steering cooler.
7. Remove the power steering cooler pipe/hose from the vehicle.

### Installation Procedure

1. Position the power steering cooler pipe/hose to the vehicle.
2. Connect the power steering cooler pipe/hose to the power steering cooler.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the power steering cooler pipe/hose to frame retaining bolt.

Tighten
Tighten the bolts to 4 N·m (35 lb in).

4. Connect the power steering cooler pipe/hose to the power steering lines.
5. Install the front air deflector. Refer to Front Air Deflector Replacement.
6. Lower the vehicle.
7. Remove the drain pan from under the vehicle.
8. Bleed the power steering system. Refer to Power Steering System Bleeding.