For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel compartment. Refer to Instrument Cluster Gages Inoperative.
2. Release the screws securing the Instrument Integration Module to the module bracket.
3. Disconnect the electrical connectors.

### Installation Procedure

1. Connect the electrical connectors.
2. Install the module to the bracket.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the screws that secure the module to the bracket.

Tighten
Tighten the screws to 2 N·m (18 lb in).

4. Install the instrument panel compartment. Refer to Instrument Cluster Gages Inoperative.
5. Re-program the module. Refer to Control Module References.