For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front seats. Refer to Driver or Passenger Seat Replacement .
2. Remove the front seat switch trim panel assembly. Refer to Power Seat Switch Replacement .
3. Recalibrate SIR passenger pressence system. After any parts of seat cushion or passenger presence system is removed, refer to Inflatable Restraint Sensing and Diagnostic Module Programming and Setup .

1 | Front Seat Frame Retaining Nut (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 9 N·m(80 lb in)
2 | Front Seat Cushion Cover

#### Procedure:

1. Disconnect the electrical connector and remove the seat cushion.
2. Loose J-channel retainer and two side clips. Remove the front seat cushion cover. Notice the alignment of the cover and the seat cushion when installing the seat cushion cover.

3 | Front Seat Blower Retaining Bolt (Qty: 2) Tighten 3N·m(25 lb in)
4 | Front Seat Blower Tip Remove the blower from heater directly.
5 | Front Seat Heater Tip Thread the heater through the front seat cushion frame and pad, separate the heater from the front seat cushion and pad.
6 | Front Seat Cushion and Pad, Frame Tip Separate the front seat cushion frame and pad.