For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
Schematic Reference: Fog Lights Schematics Connector End View Reference: Master Electrical Component List
1 | Did you perform the Diagnostic System Check - Vehicle? | Go to Step 2 | Go to Diagnostic System Check - Vehicle
2 | Do the front fog lamps operate properly? | Go to Step 3 | Go to Fog Lamps Inoperative
3 | Inspect for poor connections at the harness connector of the instrument panel cluster (IPC). Refer to Testing for Intermittent Conditions and Poor Connections and Connector Repairs . Did you find and correct the condition? | Go to Step 5 | Go to Step 4
4 | Replace the IPC. Refer to Control Module References for replacement, setup, and programming. Did you complete the replacement? | Go to Step 5 | --
5 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 2