For 1990-2009 cars

This master DTC list includes all applicable DTCs in alphanumeric order with descriptors.

The GM LAN modules on this vehicle also support DTC Symptom information. Refer to DTC Symptom Description for additional information on DTC Symptoms.

DTC | DTC Descriptor | Module that sets the DTC | Diagnostic Procedure
--- | --- | --- | ---
B0012 | Driver Frontal Deployment Loop Stage 1 | Sensing and Diagnostic Module (SDM) | DTC B0012 or B0013
B0013 | Driver Frontal Deployment Loop Stage 2 | Sensing and Diagnostic Module (SDM) | DTC B0012 or B0013
B0014 | Left Front Side Deployment Loop | Sensing and Diagnostic Module (SDM) | DTC B0014
B0015 | Left Front Pretensioner Deployment Loop | Sensing and Diagnostic Module (SDM) | DTC B0015
B0016 | Left Roof Rail Deployment Loop | Sensing and Diagnostic Module (SDM) | DTC B0016
B0019 | Passenger Frontal Deployment Loop Stage 1 | Sensing and Diagnostic Module (SDM) | DTC B0019 or B0020
B0020 | Passenger Frontal Deployment Loop Stage 2 | Sensing and Diagnostic Module (SDM) | DTC B0019 or B0020
B0021 | Right Front Side Deployment Loop | Sensing and Diagnostic Module (SDM) | DTC B0021
B0022 | Right Front Pretensioner Deployment Loop | Sensing and Diagnostic Module (SDM) | DTC B0022
B0023 | Right Roof Rail Deployment Loop | Sensing and Diagnostic Module (SDM) | DTC B0023
B0052 | Deployment Commanded | Sensing and Diagnostic Module (SDM) | DTC B0052
B0053 | Deployment Commanded With Loop DTCs Present | Sensing and Diagnostic Module (SDM) | DTC B0053
B0055 | Side Airbag Deployment Commanded | Sensing and Diagnostic Module (SDM) | DTC B0055
B0083 | Front End Sensor 1 | Sensing and Diagnostic Module (SDM) | DTC B0083 or B0084
B0084 | Front End Sensor 2 | Sensing and Diagnostic Module (SDM) | DTC B0083 or B0084
B0085 | Left Front Side Impact Sensor (SIS) | Sensing and Diagnostic Module (SDM) | DTC B0085
B0086 | Right Front Side Impact Sensor (SIS) | Sensing and Diagnostic Module (SDM) | DTC B0086
B0158 | Outside Air Temperature Circuit | HVAC | DTC B0158 or B0163
B0163 | Passenger Compartment Temperature Sensor Circuit | HVAC | DTC B0158 or B0163
B0183 | Solar Load Sensor 1 Circuit | HVAC | DTC B0183 or B0188
B0188 | Solar Load Sensor 2 Circuit | HVAC | DTC B0183 or B0188
B0248 | Air Flow Control 3 Circuit | HVAC | DTC B0248, B0268, B0408, B0418, B0428, or B3531
B0268 | Air Flow Control 7 Circuit | HVAC | DTC B0248, B0268, B0408, B0418, B0428, or B3531
B0408 | Temperature Control 1 Circuit | HVAC | DTC B0248, B0268, B0408, B0418, B0428, or B3531
B0413 | Temperature Control 1 Feedback Circuit | HVAC | DTC B0413, B0423, B0433, B3761, B3773, or B3782
B0418 | Temperature Control 2 Circuit | HVAC | DTC B0248, B0268, B0408, B0418, B0428, or B3531
B0423 | Temperature Control 2 Feedback Circuit | HVAC | DTC B0413, B0423, B0433, B3761, B3773, or B3782
B0428 | Temperature Control 3 Circuit | HVAC | DTC B0248, B0268, B0408, B0418, B0428, or B3531
B0433 | Temperature Control 3 Feedback Circuit | HVAC | DTC B0413, B0423, B0433, B3761, B3773, or B3782
B0996 | Vehicle Electronic Control Unit (ECU) VIN Check Error | VTD | DTC B0996
B1000 | Electronic Control Unit (ECU) Performance | Audio Amplifier, DDM, DDS, DHL, DPM, DRR, ESC, HVAC, IPC, IPM, LRDM, PDM, Radio, RCDLR, RIM, RRDM, SCLCM, SDM | DTC B1000
B1001 | Option Configuration Error | Radio | DTC B1001 in Entertainment
Sensing and Diagnostic Module (SDM) | DTC B1001
B1010 | System Sensors Data Mismatch | DHL | DTC B1010
B1015 | Vehicle Identification Number (VIN) Information Error | VTD | DTC B1015
B1019 | System Configuration Error | Sensing and Diagnostic Module (SDM) | DTC B1019
B1325 | Device Power Circuit | AMP, DDM, DDS, DHL, DPM, HVAC, IPC, IPM, LRDM, PDM, Radio, RCDLR, RIM, RRDM, SCLCM, TVT | DTC B1325
Device Power 1 (low current 1) Circuit | Sensing and Diagnostic Module (SDM) | DTC B1325
B1335 | Device Power 3 Circuit Range/Performance | MSM | DTC B1335
B1370 | Device Ignition 1 (ON and START) Circuit | RCDLR | DTC B1370
Sensing and Diagnostic Module (SDM) | DTC B1370
B1380 | Device Ignition ACCESSORY Circuit | IPM | DTC B1380
B1385 | Device Ignition START Circuit | IPM | DTC B1385
B1422 | Device Power Mode Error | IPM | DTC B1422
B1440 | Power Mode Master Input Circuits Mismatch | RCDLR | DTC B1440
B1457 | AHLD Left Servo Driver Terminal 3 Circuit | DHL | DTC B1457
B1458 | AHLD Left Servo Driver Terminal 4 Circuit | DHL | DTC B1458
B1459 | AHLD Right Servo Driver Terminal 3 Circuit | DHL | DTC B1459
B1460 | AHLD Right Servo Driver Terminal 4 Circuit | DHL | DTC B1460
B1516 | Battery Current Sensor Performance | IPM | DTC B1516
B1517 | Battery Voltage | IPM | DTC B1517
B1560 | Mirror Right Control Switch Circuit | DDS | DTC B1560, B1565, B1570, or B1575
B1565 | Mirror Left Control Switch Circuit | DDS | DTC B1560, B1565, B1570, or B1575
B1570 | Mirror Up Control Switch Circuit | DDS | DTC B1560, B1565, B1570, or B1575
B1575 | Mirror Down Control Switch Circuit | DDS | DTC B1560, B1565, B1570, or B1575
B1580 | Mirror Horizontal Position Sensor Circuit | DDM, PDM | DTC B1580 or B1590
B1590 | Mirror Vertical Position Sensor Circuit | DDM, PDM | DTC B1580 or B1590
B1715 | Outside Mirror Power Fold Control Switch Circuit | DDS | DTC B1715
B1735 | Left Front Seat Front Up Switch Circuit | MSM | DTC B1735, B1740, B1745, B1750, B1755, B1760, B1815, B1820, B1830, B1835, B1840, B1845, B1940, or B1945
B1740 | Left Front Seat Front Down Switch Circuit | MSM | DTC B1735, B1740, B1745, B1750, B1755, B1760, B1815, B1820, B1830, B1835, B1840, B1845, B1940, or B1945
B1745 | Left Front Seat Rear Up Switch Circuit | MSM | DTC B1735, B1740, B1745, B1750, B1755, B1760, B1815, B1820, B1830, B1835, B1840, B1845, B1940, or B1945
B1750 | Left Front Seat Rear Down Switch Circuit | MSM | DTC B1735, B1740, B1745, B1750, B1755, B1760, B1815, B1820, B1830, B1835, B1840, B1845, B1940, or B1945
B1755 | Left Front Seat Assembly Forward Switch Circuit | MSM | DTC B1735, B1740, B1745, B1750, B1755, B1760, B1815, B1820, B1830, B1835, B1840, B1845, B1940, or B1945
B1760 | Left Front Seat Assembly Rearward Switch Circuit | MSM | DTC B1735, B1740, B1745, B1750, B1755, B1760, B1815, B1820, B1830, B1835, B1840, B1845, B1940, or B1945
B1815 | Left Front Seat Recline Forward Switch Circuit | MSM | DTC B1735, B1740, B1745, B1750, B1755, B1760, B1815, B1820, B1830, B1835, B1840, B1845, B1940, or B1945
B1820 | Left Front Seat Recline Rearward Switch Circuit | MSM | DTC B1735, B1740, B1745, B1750, B1755, B1760, B1815, B1820, B1830, B1835, B1840, B1845, B1940, or B1945
B1825 | Seat Recline Position Sensor Circuit | MSM | DTC B1825, B1850, B1860, B2355, B2365, or B2375
B1830 | Left Front Seat Lumbar Forward Switch Circuit | MSM | DTC B1735, B1740, B1745, B1750, B1755, B1760, B1815, B1820, B1830, B1835, B1840, B1845, B1940, or B1945
B1835 | Left Front Seat Lumbar Rearward Switch Circuit | MSM | DTC B1735, B1740, B1745, B1750, B1755, B1760, B1815, B1820, B1830, B1835, B1840, B1845, B1940, or B1945
B1840 | Left Front Seat Lumbar Up Switch Circuit | MSM | DTC B1735, B1740, B1745, B1750, B1755, B1760, B1815, B1820, B1830, B1835, B1840, B1845, B1940, or B1945
B1845 | Left Front Seat Lumbar Down Switch Circuit | MSM | DTC B1735, B1740, B1745, B1750, B1755, B1760, B1815, B1820, B1830, B1835, B1840, B1845, B1940, or B1945
B1850 | Seat Lumbar Horizontal Position Sensor Circuit | MSM | DTC B1825, B1850, B1860, B2355, B2365, or B2375
B1860 | Seat Lumbar Vertical Position Sensor Circuit | MSM | DTC B1825, B1850, B1860, B2355, B2365, or B2375
B2355 | Seat Front Vertical Position Sensor Circuit | MSM | DTC B1825, B1850, B1860, B2355, B2365, or B2375
B2365 | Seat Rear Vertical Position Sensor Circuit | MSM | DTC B1825, B1850, B1860, B2355, B2365, or B2375
B2375 | Seat Assembly Horizontal Position Sensor Circuit | MSM | DTC B1825, B1850, B1860, B2355, B2365, or B2375
B2496 | Outside Air Quality Sensor 2 Circuit | HVAC | DTC B2496 or B3843
B2645 | Ambient Light Sensor Circuit | HVAC | DTC B2645
B2667 | AHLD Left Servo Driver Terminal 1 Circuit | DHL | DTC B2667
B2672 | AHLD Left Servo Driver Terminal 2 Circuit | DHL | DTC B2672
B2677 | AHLD Right Servo Driver Terminal 1 Circuit | DHL | DTC B2677
B2682 | AHLD Right Servo Driver Terminal 2 Circuit | DHL | DTC B2682
B2697 | Headlamp Washer Request Circuit | IPM | DTC B2697
B2710 | Shift Lock Control Circuit | RCDLR | DTC B2710
B2732 | Trunk Release Switch Circuit Low | RIM | DTC B2732
B2755 | Left Front Memory 1 Selector Switch Circuit | DDS |
B2765 | Memory Setting Switch Circuit Failure | DDS |
B2760 | Left Front Memory 2 Selector Switch Circuit | DDS |
B2730 | Trunk Release Switch Circuit | DDS |
B2860 | Telescope Position Sensor | MSM | DTC B2860
B2880 | Tilt Position Sensor | MSM | DTC B2880
B2923 | Content Theft System Inclination Sensor Signal Circuit | RIM | DTC B2923
B3006 | Hood Ajar Circuit | IPM | DTC B3006
B3062 | Door Key Lock Switch Circuit | DDM | DTC B3062 or B3067
B3067 | Door Key Unlock Switch Circuit | DDM | DTC B3062 or B3067
B3089 | Content Theft System Intrusion Sensor Signal Circuit | IPM | DTC B3089
B3119 | Keyless Entry Antenna 1 Performance | Easy Key | DTC B3119
B3120 | Keyless Entry Antenna 2 Performance | Easy Key | DTC B3120
B3121 | Keyless Entry Antenna 3 Performance | Easy Key | DTC B3121
B3122 | Keyless Entry Antenna 4 Performance | Easy Key | DTC B3122
B3123 | Keyless Entry Antenna 5 and 6 Performance | Easy Key | DTC B3123
B3140 | Unlock Switch Circuit | DDS/PDM | DTC B3140 or B3150
B3150 | Lock Switch Circuit | DDS/PDM | DTC B3140 or B3150
B3160 | Window Up Switch Circuit | PDM, LRDM, RRDM | DTC B3160 or B3165
B3165 | Window Down Switch Circuit | PDM, LRDM, RRDM | DTC B3160 or B3165
B3275 | Window Express Up or Down Circuit (at door) | PDM, LRDM, RRDM | DTC B3275
B3375 | Left Front Window Up Switch Circuit | DDS | DTC B3375, B3380, B3385, B3390, B3395, B3450, B3455, B3460, B3485, B3490, B3495, or B3500
B3380 | Left Front Window Down Switch Circuit | DDS | DTC B3375, B3380, B3385, B3390, B3395, B3450, B3455, B3460, B3485, B3490, B3495, or B3500
B3385 | Right Front Window Up Switch Circuit | DDS | DTC B3375, B3380, B3385, B3390, B3395, B3450, B3455, B3460, B3485, B3490, B3495, or B3500
B3390 | Right Front Window Down Switch Circuit | DDS | DTC B3375, B3380, B3385, B3390, B3395, B3450, B3455, B3460, B3485, B3490, B3495, or B3500
B3395 | Left Rear Window Up Switch Circuit | DDS | DTC B3375, B3380, B3385, B3390, B3395, B3450, B3455, B3460, B3485, B3490, B3495, or B3500
B3410 | AHLD Front Axle Sensor Signal Circuit | DHL | DTC B3410
B3420 | AHLD Rear Axle Sensor Signal Circuit | DHL | DTC B3420
B3450 | Left Rear Window Down Switch Circuit | DDS | DTC B3375, B3380, B3385, B3390, B3395, B3450, B3455, B3460, B3485, B3490, B3495, or B3500
B3455 | Right Rear Window Up Switch Circuit | DDS | DTC B3375, B3380, B3385, B3390, B3395, B3450, B3455, B3460, B3485, B3490, B3495, or B3500
B3460 | Right Rear Window Down Switch Circuit | DDS | DTC B3375, B3380, B3385, B3390, B3395, B3450, B3455, B3460, B3485, B3490, B3495, or B3500
B3485 | Left Front Window Express Up Circuit | DDS | DTC B3375, B3380, B3385, B3390, B3395, B3450, B3455, B3460, B3485, B3490, B3495, or B3500
B3490 | Right Front Window Express Up Circuit | DDS | DTC B3375, B3380, B3385, B3390, B3395, B3450, B3455, B3460, B3485, B3490, B3495, or B3500
B3495 | Left Rear Window Express Up Circuit | DDS | DTC B3375, B3380, B3385, B3390, B3395, B3450, B3455, B3460, B3485, B3490, B3495, or B3500
B3500 | Right Rear Window Express Up Circuit | DDS | DTC B3375, B3380, B3385, B3390, B3395, B3450, B3455, B3460, B3485, B3490, B3495, or B3500
B3505 | Right Rear Window Express Down Circuit | DDS |
B3510 | Right Front Window Express Down Circuit | DDS |
B3515 | Left Rear Window Express Down Circuit | DDS |
B3520 | Right Rear Window Express Down Circuit | DDS |
B3525 | Window Lockout Switch Circuit | DDS | DTC B3525
B3531 | Air Flow Control 10 Circuit | HVAC | DTC B0248, B0268, B0408, B0418, B0428, or B3531
B3600 | Passenger Compartment Dimming Request Signal Circuit | IPM | DTC B3600
B3622 | Steering Wheel Controls Signal Circuit | IPM | DTC B3622
B3761 | Air Flow Control 3 Feedback Circuit | HVAC | DTC B0248, B0268, B0408, B0418, B0428, or B3531
B3773 | Air Flow Control 7 Feedback Circuit | HVAC | DTC B0248, B0268, B0408, B0418, B0428, or B3531
B3782 | Air Flow Control 10 Feedback Circuit | HVAC | DTC B0248, B0268, B0408, B0418, B0428, or B3531
B3794 | Cruise Control Function Request Circuit | IPM | DTC B3794
B3832 | Window Express Up System/ Function Not Initialized | DDM/PDM/ LRDM/RRDM | DTC B3832
B3843 | Outside Air Quality Sensor 1 Circuit | HVAC | DTC B2496 or B3843
B3849 | Exterior Door Handle Switch Circuit | DDM/PDM | DTC B1474 or B3849
B3933 | Air Conditioning (A/C) Evaporator Temperature Sensor Circuit | HVAC | DTC B3933
C0035 | Left Front Wheel Speed Sensor Circuit | EBCM | DTC C0035-C0051
C0040 | Right Front Wheel Speed Sensor Circuit | EBCM | DTC C0035-C0051
C0045 | Left Rear Wheel Speed Sensor Circuit | EBCM | DTC C0035-C0051
C0050 | Right Rear Wheel Speed Sensor Circuit | EBCM | DTC C0035-C0051
C0110 | Pump Motor Circuit | EBCM | DTC C0110
C0136 | Regular Brake System Pressure Circuit | EBCM | DTC C0136
C0137 | Regular Brake System Pressure Circuit Range | EBCM | DTC C0137
C0161 | Antilock Brake System (ABS)/ Traction Control System (TCS) Brake Switch Circuit | EBCM | DTC C0161
C0179 | Lateral Accelerometer Circuit | EBCM | DTC C0179
C186 | Lateral Accelerometer Circuit | EBCM | DTC C0186
C0192 | All Wheel Drive (AWD)/Four Wheel Drive (4WD) Reference Accelerometer Circuit | EBCM | DTC C0192
C0196 | Yaw Rate Circuit | EBCM | DTC C0196
C0228 | Left Rear Antilock Brake System (ABS) Channel in Release Too Long | EBCM | DTC C0220-C0229
C0229 | Right Rear Antilock Brake System (ABS) Channel in Release Too Long | EBCM | DTC C0220-C0229
C0240 | Powertrain Control Module (PCM) Traction Control Not Allowed | EBCM | DTC C0240
C0242 | Powertrain Control Module (PCM) Indicated TCS Malfunction | EBCM | DTC C0242
C0249 | Left Normal Force Error | EBCM | DTC C0249 or C0250
C0250 | Right Normal Force Error | EBCM | DTC C0249 or C0250
C0252 | Vehicle Stability Enhancement System (VSES) Sensors Uncorrelated | EBCM | DTC C0252
C0253 | Centering Error | EBCM | DTC C0253
C0267 | Low Brake Fluid Indicated | EBCM | DTC C0267
C0277 | Brake Pedal Position Sensor Circuit | IPM | DTC C0277
C0278 | Brake Pedal Position Sensor Not Calibrated | IPM | DTC C0278
C0281 | Dynamic Rear Proportioning (DRP) Performance | EBCM | DTC C0281
C0450 | Steering Assist Control Actuator Circuit | EBCM | DTC C0450
C0550 | Electronic Control Unit (ECU) Performance | EBCM | DTC C0550
ESC | DTC C0550
C0551 | Option Configuration Error | EBCM | DTC C0551
C0558 | Calibration Data Not Programmed | ESC | DTC C0558
C0561 | System Disabled Information Stored | EBCM | DTC C0561
C0565 | Vehicle Identification Number (VIN) Information Error | EBCM | DTC C0565
C0575 | Left Front Actuator Circuit | ESC | DTC C0575, C0580, C0585, or C0590
C0580 | Right Front Actuator Circuit | ESC | DTC C0575, C0580, C0585, or C0590
C0585 | Left Rear Actuator Circuit | ESC | DTC C0575, C0580, C0585, or C0590
C0590 | Right Rear Actuator Circuit | ESC | DTC C0575, C0580, C0585, or C0590
C0615 | Left Front Position Sensor Circuit | ESC | DTC C0615, C0620, C0625, or C0630
C0620 | Right Front Position Sensor Circuit | ESC | DTC C0615, C0620, C0625, or C0630
C0625 | Left Rear Position Sensor Circuit | ESC | DTC C0615, C0620, C0625, or C0630
C0630 | Right Rear Position Sensor Circuit | ESC | DTC C0615, C0620, C0625, or C0630
C0660 | Level Control Exhaust Valve Circuit | ESC | DTC C0660
C0696 | Position Sensor Overcurrent (5-volt supply) | ESC | DTC C0696
C0710 | Steering Position Signal | EBCM | DTC C0710
C0712 | Level Control Compressor Relay Circuit | ESC | DTC C0712
C0750 | Left Front Low Tire Pressure Sensor | RCDLR | DTC C0750, C0755, C0760, or C0765
C0755 | Right Front Low Tire Pressure Sensor | RCDLR | DTC C0750, C0755, C0760, or C0765
C0760 | Left Rear Low Tire Pressure Sensor | RCDLR | DTC C0750, C0755, C0760, or C0765
C0765 | Right Rear Low Tire Pressure Sensor | RCDLR | DTC C0750, C0755, C0760, or C0765
C0774 | Tire Pressure System Performance Poor | EBCM |
C0820 | Device Ground Circuit | EBCM | DTC C0820
C0870 | Device Voltage Reference Output Circuit | EBCM | DTC C0870
Brake Pedal Position Sensor Voltage Reference Circuit | IPM | DTC C0870
C0895 | Device Voltage | ESC | DTC C0895
C0899 | Device Voltage Low | EBCM | DTC C0899
C0900 | Device Voltage High | EBCM | DTC C0900
P0008 | Engine Position System Performance Bank 1 | ECM | DTC P0008 for the 3.6L (LY7) engine
P0009 | Engine Position System Performance Bank 2 | ECM | DTC P0009 for the 3.6L (LY7) engine
P0010 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit Bank 1 | ECM | DTC P0010, P0013, P0020, or P0023 for the 3.6L (LY7) engine DTC P0010, P0011, P0013, P0014, P0020, P0021, P0023, or P0024 for the 4.6L (LH2) engine
P0011 | Intake Camshaft Position (CMP) System Performance Bank 1 | ECM | DTC P0011, P0014, P0021, or P0024 for the 3.6L (LY7) engine DTC P0010, P0011, P0013, P0014, P0020, P0021, P0023, or P0024 for the 4.6L (LH2) engine
P0013 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit Bank 1 | ECM | DTC P0010, P0013, P0020, or P0023 for the 3.6L (LY7) engine DTC P0010, P0011, P0013, P0014, P0020, P0021, P0023, or P0024 for the 4.6L (LH2) engine
P0014 | Exhaust Camshaft Position (CMP) System Performance Bank 1 | ECM | DTC P0011, P0014, P0021, or P0024 for the 3.6L (LY7) engine DTC P0010, P0011, P0013, P0014, P0020, P0021, P0023, or P0024 for the 4.6L (LH2) engine
P0016 | Crankshaft Position (CKP) - Intake Camshaft Position (CMP) Correlation Bank 1 | ECM | DTC P0016, P0017, P0018, or P0019 for the 3.6L (LY7) engine DTC P0016, P0017, P0018, or P0019 for the 4.6L (LH2) engine
P0017 | Crankshaft Position (CKP) - Exhaust Camshaft Position (CMP) Correlation Bank 1 | ECM | DTC P0016, P0017, P0018, or P0019 for the 3.6L (LY7) engine DTC P0016, P0017, P0018, or P0019 for the 4.6L (LH2) engine
P0018 | Crankshaft Position (CKP) - Intake Camshaft Position (CMP) Correlation Bank 2 | ECM | DTC P0016, P0017, P0018, or P0019 for the 3.6L (LY7) engine DTC P0016, P0017, P0018, or P0019 for the 4.6L (LH2) engine
P0019 | Crankshaft Position (CKP) - Exhaust Camshaft Position (CMP) Correlation Bank 2 | ECM | DTC P0016, P0017, P0018, or P0019 for the 3.6L (LY7) engine DTC P0016, P0017, P0018, or P0019 for the 4.6L (LH2) engine
P0020 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit Bank 2 | ECM | DTC P0010, P0013, P0020, or P0023 for the 3.6L (LY7) engine DTC P0010, P0011, P0013, P0014, P0020, P0021, P0023, or P0024 for the 4.6L (LH2) engine
P0021 | Intake Camshaft Position (CMP) System Performance Bank 2 | ECM | DTC P0011, P0014, P0021, or P0024 for the 3.6L (LY7) engine DTC P0010, P0011, P0013, P0014, P0020, P0021, P0023, or P0024 for the 4.6L (LH2) engine
P0023 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit Bank 2 | ECM | DTC P0010, P0013, P0020, or P0023 for the 3.6L (LY7) engine DTC P0010, P0011, P0013, P0014, P0020, P0021, P0023, or P0024 for the 4.6L (LH2) engine
P0024 | Exhaust Camshaft Position (CMP) System Performance Bank 2 | ECM | DTC P0011, P0014, P0021, or P0024 for the 3.6L (LY7) engine DTC P0010, P0011, P0013, P0014, P0020, P0021, P0023, or P0024 for the 4.6L (LH2) engine
P0030 | HO2S Heater Control Circuit Bank 1 Sensor 1 | ECM | DTC P0030, P0036, P0050, or P0056 for the 3.6L (LY7) engine DTC P0030, P0036, P0053, P0054, P0135, or P0141 for the 4.6L (LH2) engine
P0031 | HO2S Heater Control Circuit Low Voltage Bank 1 Sensor 1 | ECM | DTC P0031, P0037, P0051, or P0057 for the 3.6L (LY7) engine
P0032 | HO2S Heater Control Circuit High Voltage Bank 1 Sensor 1 | ECM | DTC P0032, P0038, P0052, or P0058 for the 3.6L (LY7) engine
P0036 | HO2S Heater Control Circuit Bank 1 Sensor 2 | ECM | DTC P0030, P0036, P0050, or P0056 for the 3.6L (LY7) engine DTC P0030, P0036, P0053, P0054, P0135, or P0141 for the 4.6L (LH2) engine
P0037 | HO2S Heater Control Circuit Low Voltage Bank 1 Sensor 2 | ECM | DTC P0031, P0037, P0051, or P0057 for the 3.6L (LY7) engine
P0038 | HO2S Heater Control Circuit High Voltage Bank 1 Sensor 2 | ECM | DTC P0032, P0038, P0052, or P0058 for the 3.6L (LY7) engine
P0050 | HO2S Heater Control Circuit Bank 2 Sensor 1 | ECM | DTC P0030, P0036, P0050, or P0056 for the 3.6L (LY7) engine DTC P0030, P0036, P0053, P0054, P0135, or P0141 for the 4.6L (LH2) engine
P0051 | HO2S Heater Control Circuit Low Voltage Bank 2 Sensor 1 | ECM | DTC P0031, P0037, P0051, or P0057 for the 3.6L (LY7) engine
P0052 | HO2S Heater Control Circuit High Voltage Bank 2 Sensor 1 | ECM | DTC P0032, P0038, P0052, or P0058 for the 3.6L (LY7) engine
P0053 | HO2S Heater Resistance Bank 1 Sensor 1 | ECM | DTC P0053 for the 3.6L (LY7) engine DTC P0030, P0036, P0053, P0054, P0135, or P0141 for the 4.6L (LH2) engine
P0054 | HO2S Heater Resistance Bank 1 Sensor 2 | ECM | DTC P0030, P0036, P0053, P0054, P0135, or P0141 for the 4.6L (LH2) engine
P0056 | HO2S Heater Control Circuit Bank 2 Sensor 2 | ECM | DTC P0030, P0036, P0050, or P0056 for the 3.6L (LY7) engine DTC P0050, P0056, P0059, P0060, P0155, or P0161 for the 4.6L (LH2) engine
P0057 | HO2S Heater Control Circuit Low Voltage Bank 2 Sensor 2 | ECM | DTC P0031, P0037, P0051, or P0057 for the 3.6L (LY7) engine
P0058 | HO2S Heater Control Circuit High Voltage Bank 2 Sensor 2 | ECM | DTC P0032, P0038, P0052, or P0058 for the 3.6L (LY7) engine
P0059 | HO2S Heater Resistance Bank 2 Sensor 1 | ECM | DTC P0059 for the 3.6L (LY7) engine
HO2S Heater Resistance Bank 2 Sensor 1 | ECM | DTC P0050, P0056, P0059, P0060, P0155, or P0161 for the 4.6L (LH2) engine
P0060 | HO2S Heater Resistance Bank 2 Sensor 2 | ECM | DTC P0050, P0056, P0059, P0060, P0155, or P0161 for the 4.6L (LH2) engine
P0068 | Throttle Body Airflow Performance | ECM | DTC P0068 or P0121 for the 4.6L (LH2) engine
P0101 | Mass Air Flow (MAF) Sensor Performance | ECM | DTC P0101 for the 3.6L (LY7) engine DTC P0101 or P1101 for the 4.6L (LH2) engine
P0102 | Mass Air Flow (MAF) Sensor Circuit Low Voltage | ECM | DTC P0102 for the 3.6L (LY7) engine DTC P0102 or P0103 for the 4.6L (LH2) engine
P0103 | Mass Air Flow (MAF) Sensor Circuit High Voltage | ECM | DTC P0102 for the 3.6L (LY7) engine DTC P0102 or P0103 for the 4.6L (LH2) engine
P0106 | Manifold Absolute Pressure (MAP) Sensor Performance | ECM | DTC P0106 for the 4.6L (LH2) engine
P0107 | Manifold Absolute Pressure (MAP) Sensor Circuit Low Voltage | ECM | DTC P0107 or P0108 for the 4.6L (LH2) engine
P0108 | Manifold Absolute Pressure (MAP) Sensor Circuit High Voltage | ECM | DTC P0107 or P0108 for the 4.6L (LH2) engine
P0111 | Intake Air Temperature (IAT) Sensor Circuit Performance | ECM | DTC P0111 for the 3.6L (LY7) engine
P0112 | Intake Air Temperature (IAT) Sensor Circuit Low Voltage | ECM | DTC P0112 for the 3.6L (LY7) engine DTC P0112 or P0113 for the 4.6L (LH2) engine
P0113 | Intake Air Temperature (IAT) Sensor Circuit High Voltage | ECM | DTC P0112 for the 3.6L (LY7) engine DTC P0112 or P0113 for the 4.6L (LH2) engine
P0116 | Engine Coolant Temperature (ECT) Sensor Performance | ECM | DTC P0116 for the 3.6L (LY7) engine DTC P0116 for the 4.6L (LH2) engine
P0117 | Engine Coolant Temperature (ECT) Sensor Circuit Low Voltage | ECM | DTC P0117 for the 3.6L (LY7) engine DTC P0117 or P0118 for the 4.6L (LH2) engine
P0118 | Engine Coolant Temperature (ECT) Sensor Circuit High Voltagel | ECM | DTC P0118 for the 3.6L (LY7) engine DTC P0117 or P0118 for the 4.6L (LH2) engine
P0119 | Engine Coolant Temperature (ECT) Sensor Circuit Intermittent Failure | ECM | DTC P0119
P0120 | Throttle Position (TP) Sensor Circuit | TCM | DTC P0120 for the 5L40-E transmission
Throttle Position (TP) Sensor 1 Circuit | ECM | DTC P0120, P0122, P0123, P0220, P0222, P0223, or P2135 for the 4.6L (LH2) engine
P0121 | Throttle Position (TP) Sensor 1 Performance | ECM | DTC P0121 for the 3.6L (LY7) engine DTC P0068 or P0121 for the 4.6L (LH2) engine
P0122 | Throttle Position (TP) Sensor 1 Circuit Low Voltage | ECM | DTC P0122 for the 3.6L (LY7) engine DTC P0120, P0122, P0123, P0220, P0222, P0223, or P2135 for the 4.6L (LH2) engine
P0123 | Throttle Position (TP) Sensor 1 Circuit High Voltage | ECM | DTC P0123 for the 3.6L (LY7) engine DTC P0120, P0122, P0123, P0220, P0222, P0223, or P2135 for the 4.6L (LH2) engine
P0125 | Engine Coolant Temperature (ECT) Insufficient for Closed Loop Fuel Control | ECM | DTC P0125 for the 3.6L (LY7) engine
P0128 | Engine Coolant Temperature (ECT) Below Thermostat Regulating Temperature | ECM | DTC P0128 for the 3.6L (LY7) engine
P0130 | HO2S Circuit Bank 1 Sensor 1 | ECM | DTC P0130 or P0150 for the 3.6L (LY7) engine
P0131 | HO2S Circuit Low Voltage Bank 1 Sensor 1 | ECM | DTC P0131 or P0151 for the 3.6L (LY7) engine DTC P0131, P0132, P0137, or P0138 for the 4.6L (LH2) engine
P0132 | HO2S Circuit High Voltage Bank 1 Sensor 1 | ECM | DTC P0132 or P0152 for the 3.6L (LY7) engine DTC P0131, P0132, P0137, or P0138 for the 4.6L (LH2) engine
P0133 | HO2S Slow Response Bank 1 Sensor 1 | ECM | DTC P0133 or P0153 for the 3.6L (LY7) engine DTC P0133, P0134, P0140, P1133, or P2A00 for the 4.6L (LH2) engine
P0134 | HO2S Circuit Insufficient Activity Bank 1 Sensor 1 | ECM | DTC P0133, P0134, P0140, P1133, or P2A00 for the 4.6L (LH2) engine
P0135 | HO2S Heater Performance Bank 1 Sensor 1 | ECM | DTC P0135 or P0155 for the 3.6L (LY7) engine DTC P0030, P0036, P0053, P0054, P0135, or P0141 for the 4.6L (LH2) engine
P0137 | HO2S Circuit Low Voltage Bank 1 Sensor 2 | ECM | DTC P0137 or P0157 for the 3.6L (LY7) engine DTC P0131, P0132, P0137, or P0138 for the 4.6L (LH2) engine
P0138 | HO2S Circuit High Voltage Bank 1 Sensor 2 | ECM | DTC P0138 or P0158 for the 3.6L (LY7) engine DTC P0131, P0132, P0137, or P0138 for the 4.6L (LH2) engine
P0139 | HO2S Slow Response Bank 1 Sensor 2 | ECM | DTC P0139, P013A, P013C, P013E, P014A, or P0159 for the 3.6L (LY7) engine
P013A | HO2S Slow Response Bank 1 Sensor 2 | ECM | DTC P0139, P013A, P013C, P013E, P014A, or P0159 for the 3.6L (LY7) engine
P013C | HO2S Slow Response Bank 2 Sensor 2 | ECM | DTC P0139, P013A, P013C, P013E, P014A, or P0159 for the 3.6L (LY7) engine
P013E | HO2S Slow Response Bank 1 Sensor 2 | ECM | DTC P0139, P013A, P013C, P013E, P014A, or P0159 for the 3.6L (LY7) engine
P0140 | HO2S Circuit Insufficient Activity Bank 1 Sensor 2 | ECM | DTC P0140 or P0160 for the 3.6L (LY7) engine DTC P0133, P0134, P0140, P1133, or P2A00 for the 4.6L (LH2) engine
P0141 | HO2S Heater Performance Bank 1 Sensor 2 | ECM | DTC P0141 or P0161 for the 3.6L (LY7) engine DTC P0030, P0036, P0053, P0054, P0135, or P0141 for the 4.6L (LH2) engine
P014A | HO2S Slow Response Bank 2 Sensor 2 | ECM | DTC P0139, P013A, P013C, P013E, P014A, or P0159 for the 3.6L (LY7) engine
P0150 | HO2S Circuit Bank 2 Sensor 1 | ECM | DTC P0130 or P0150
P0151 | HO2S Circuit Low Voltage Bank 2 Sensor 1 | ECM | DTC P0131 or P0151 for the 3.6L (LY7) engine DTC P0151, P0152, P0157, or P0158 for the 4.6L (LH2) engine
P0152 | HO2S Circuit High Voltage Bank 2 Sensor 1 | ECM | DTC P0132 or P0152 for the 3.6L (LY7) engine DTC P0151, P0152, P0157, or P0158 for the 4.6L (LH2) engine
P0153 | HO2S Slow Response Bank 2 Sensor 1 | ECM | DTC P0133 or P0153 for the 3.6L (LY7) engine DTC P0153,P0154, P0160, P1153, or P2A03 for the 4.6L (LH2) engine
P0154 | HO2S Circuit Insufficient Activity Bank 2 Sensor 1 | ECM | DTC P0153,P0154, P0160, P1153, or P2A03 for the 4.6L (LH2) engine
P0155 | HO2S Heater Performance Bank 2 Sensor 1 | ECM | DTC P0131 or P0151 for the 3.6L (LY7) engine DTC P0050, P0056, P0059, P0060, P0155, or P0161 for the 4.6L (LH2) engine
P0157 | HO2S Circuit High Voltage Bank 2 Sensor 2 | ECM | DTC P0137 or P0157 for the 3.6L (LY7) engine DTC P0151, P0152, P0157, or P0158 for the 4.6L (LH2) engine
P0158 | HO2S Circuit High Voltage Bank 2 Sensor 2 | ECM | DTC P0138 or P0158 for the 3.6L (LY7) engine DTC P0151, P0152, P0157, or P0158 for the 4.6L (LH2) engine
P0159 | HO2S Slow Response Bank 2 Sensor 2 | ECM | DTC P0139, P013A, P013C, P013E, P014A, or P0159 for the 3.6L (LY7) engine
P0160 | HO2S Circuit Insufficient Activity Bank 2 Sensor 2 | ECM | DTC P0140 or P0160 for the 3.6L (LY7) engine DTC P0153,P0154, P0160, P1153, or P2A03 for the 4.6L (LH2) engine
P0161 | HO2S Heater Performance Bank 2 Sensor 2 | ECM | DTC P0141 or P0161 for the 3.6L (LY7) engine DTC P0050, P0056, P0059, P0060, P0155, or P0161 for the 4.6L (LH2) engine
P0171 | Fuel Trim System Lean Bank 1 | ECM | DTC P0171, P0172, P0174, or P0175 for the 4.6L (LH2) engine
P0172 | Fuel Trim System Rich Bank 1 | ECM | DTC P0171, P0172, P0174, or P0175 for the 4.6L (LH2) engine
P0174 | Fuel Trim System Lean Bank 2 | ECM | DTC P0171, P0172, P0174, or P0175 for the 4.6L (LH2) engine
P0175 | Fuel Trim System Rich Bank 2 | ECM | DTC P0171, P0172, P0174, or P0175 for the 4.6L (LH2) engine
P0201 | Injector 1 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0205, or P0206 for the 3.6L (LY7) engine DTC P0201, P0202, P0203, P0204, P0205, P0206, P0207, or P0208 for the 4.6L (LH2) engine
P0202 | Injector 2 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0205, or P0206 for the 3.6L (LY7) engine DTC P0201, P0202, P0203, P0204, P0205, P0206, P0207, or P0208 for the 4.6L (LH2) engine
P0203 | Injector 3 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0205, or P0206 for the 3.6L (LY7) engine DTC P0201, P0202, P0203, P0204, P0205, P0206, P0207, or P0208 for the 4.6L (LH2) engine
P0204 | Injector 4 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0205, or P0206 for the 3.6L (LY7) engine DTC P0201, P0202, P0203, P0204, P0205, P0206, P0207, or P0208 for the 4.6L (LH2) engine
P0205 | Injector 5 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0205, or P0206 for the 3.6L (LY7) engine DTC P0201, P0202, P0203, P0204, P0205, P0206, P0207, or P0208 for the 4.6L (LH2) engine
P0206 | Injector 6 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0205, or P0206 for the 3.6L (LY7) engine DTC P0201, P0202, P0203, P0204, P0205, P0206, P0207, or P0208 for the 4.6L (LH2) engine
P0207 | Injecto 7 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0207, or P0208 for the 4.6L (LH2) engine
P0208 | Injector 8 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0207, or P0208 for the 4.6L (LH2) engine
P0218 | Transmission Fluid Overtemperature | TCM | DTC P0218 for the 5L40-E transmission DTC P0218 for the 6L50-E transmission
P0220 | Throttle Position (TP) Sensor 2 Circuit | ECM | DTC P0120, P0122, P0123, P0220, P0222, P0223, or P2135 for the 4.6L (LH2) engine
P0221 | Throttle Position (TP) Sensor 2 Performance | ECM | DTC P0221 for the 3.6L (LY7) engine
P0222 | Throttle Position (TP) Sensor 2 Circuit Low Voltage | ECM | DTC P0222 for the 3.6L (LY7) engine DTC P0120, P0122, P0123, P0220, P0222, P0223, or P2135 for the 4.6L (LH2) engine
P0223 | Throttle Position (TP) Sensor 2 Circuit High Voltage | ECM | DTC P0223 for the 3.6L (LY7) engine DTC P0120, P0122, P0123, P0220, P0222, P0223, or P2135 for the 4.6L (LH2) engine
P0230 | Fuel Pump Relay Control Circuit | ECM | DTC P0230 for the 4.6L (LH2) engine
P0261 | Injector 1 Control Circuit Low Voltage | ECM | DTC P0261, P0264, P0267, P0270, P0273, or P0276 for the 3.6L (LY7) engine
P0262 | Injector 1 Control Circuit High Voltage | ECM | DTC P0262, P0265, P0268, P0271, P0274, or P0277 for the 3.6L (LY7) engine
P0264 | Injector 2 Control Circuit Low Voltage | ECM | DTC P0261, P0264, P0267, P0270, P0273, or P0276 for the 3.6L (LY7) engine
P0265 | Injector 2 Control Circuit High Voltage | ECM | DTC P0262, P0265, P0268, P0271, P0274, or P0277 for the 3.6L (LY7) engine
P0267 | Injector 3 Control Circuit Low Voltage | ECM | DTC P0261, P0264, P0267, P0270, P0273, or P0276 for the 3.6L (LY7) engine
P0268 | Injector 3 Control Circuit High Voltage | ECM | DTC P0262, P0265, P0268, P0271, P0274, or P0277 for the 3.6L (LY7) engine
P0270 | Injector 4 Control Circuit Low Voltage | ECM | DTC P0261, P0264, P0267, P0270, P0273, or P0276 for the 3.6L (LY7) engine
P0271 | Injector 4 Control Circuit High Voltage | ECM | DTC P0262, P0265, P0268, P0271, P0274, or P0277 for the 3.6L (LY7) engine
P0273 | Injector 5 Control Circuit Low Voltage | ECM | DTC P0261, P0264, P0267, P0270, P0273, or P0276 for the 3.6L (LY7) engine
P0274 | Injector 5 Control Circuit High Voltage | ECM | DTC P0262, P0265, P0268, P0271, P0274, or P0277 for the 3.6L (LY7) engine
P0276 | Injector 6 Control Circuit Low Voltage | ECM | DTC P0261, P0264, P0267, P0270, P0273, or P0276 for the 3.6L (LY7) engine
P0277 | Injector 6 Control Circuit High Voltage | ECM | DTC P0262, P0265, P0268, P0271, P0274, or P0277 for the 3.6L (LY7) engine
P0300 | Engine Misfire Detected | ECM | DTC P0300 for the 3.6L (LY7) engine DTC P0300 for the 4.6L (LH2) engine
P0301 | Cylinder 1 Misfire Detected | ECM | DTC P0301-P0306 for the 3.6L (LY7) engine
P0302 | Cylinder 2 Misfire Detected | ECM | DTC P0301-P0306 for the 3.6L (LY7) engine
P0303 | Cylinder 3 Misfire Detected | ECM | DTC P0301-P0306 for the 3.6L (LY7) engine
P0304 | Cylinder 4 Misfire Detected | ECM | DTC P0301-P0306 for the 3.6L (LY7) engine
P0305 | Cylinder 5 Misfire Detected | ECM | DTC P0301-P0306 for the 3.6L (LY7) engine
P0306 | Cylinder 6 Misfire Detected | ECM | DTC P0301-P0306 for the 3.6L (LY7) engine
P0315 | Crankshaft Position (CKP) System Variation Not Learned | ECM | DTC P0315 for the 4.6L (LH2) engine
P0324 | Knock Sensor (KS) Module Performance | ECM | DTC P0324 for the 3.6L (LY7) engine DTC P0324, P0325, P0326, P0327, P0328, P0330, P0332, or P0333 for the 4.6L (LH2) engine
P0325 | Knock Sensor (KS) Circuit Bank 1 | ECM | DTC P0324, P0325, P0326, P0327, P0328, P0330, P0332, or P0333 for the 4.6L (LH2) engine
P0326 | Knock Sensor (KS) Performance | ECM | DTC P0324, P0325, P0326, P0327, P0328, P0330, P0332, or P0333 for the 4.6L (LH2) engine
P0327 | Knock Sensor (KS) Circuit Low Voltage Bank 1 | ECM | DTC P0327 or P0332 for the 3.6L (LY7) engine DTC P0324, P0325, P0326, P0327, P0328, P0330, P0332, or P0333 for the 4.6L (LH2) engine
P0328 | Knock Sensor (KS) Circuit High Voltage Bank 1 | ECM | DTC P0328 or P0333 for the 3.6L (LY7) engine DTC P0324, P0325, P0326, P0327, P0328, P0330, P0332, or P0333 for the 4.6L (LH2) engine
P0330 | Knock Sensor (KS) Circuit Bank 2 | ECM | DTC P0324, P0325, P0326, P0327, P0328, P0330, P0332, or P0333 for the 4.6L (LH2) engine
P0332 | Knock Sensor (KS) Circuit Low Voltage Bank 2 | ECM | DTC P0327 or P0332 for the 3.6L (LY7) engine DTC P0324, P0325, P0326, P0327, P0328, P0330, P0332, or P0333 for the 4.6L (LH2) engine
P0333 | Knock Sensor (KS) Circuit High Voltage Bank 2 | ECM | DTC P0328 or P0333 for the 3.6L (LY7) engine DTC P0324, P0325, P0326, P0327, P0328, P0330, P0332, or P0333 for the 4.6L (LH2) engine
P0335 | Crankshaft Position (CKP) Sensor Circuit | ECM | DTC P0335 for the 3.6L (LY7) engine DTC P0335 or P0336 for the 4.6L (LH2) engine
P0336 | Crankshaft Position (CKP) Sensor Performance | ECM | DTC P0336 for the 3.6L (LY7) engine DTC P0335 or P0336 for the 4.6L (LH2) engine
P0338 | Crankshaft Position (CKP) Sensor Circuit High Duty Cycle | ECM | DTC P0338 for the 3.6L (LY7) engine
P0340 | Intake Camshaft Position (CMP) Sensor Performance Bank 1 | ECM | DTC P0340, P0341, P0345, P0346, P0365, P0366, P0390, or P0391 for the 4.6L (LH2) engine
P0341 | Intake Camshaft Position (CMP) Sensor Performance Bank 1 | ECM | DTC P0341, P0346, P0366, or P0391 for the 3.6L (LY7) engine DTC P0340, P0341, P0345, P0346, P0365, P0366, P0390, or P0391 for the 4.6L (LH2) engine
P0342 | Intake Camshaft Position (CMP) Sensor Circuit Low Voltage Bank 1 | ECM | DTC P0342, P0347, P0367, or P0392 for the 3.6L (LY7) engine
P0343 | Intake Camshaft Position (CMP) Sensor Circuit High Voltage Bank 1 | ECM | DTC P0343, P0348, P0368, or P0393 for the 3.6L (LY7) engine
P0345 | Intake Camshaft Position (CMP) Sensor Circuit Bank 2 | ECM | DTC P0340, P0341, P0345, P0346, P0365, P0366, P0390, or P0391 for the 4.6L (LH2) engine
P0346 | Intake Camshaft Position (CMP) Sensor Performance Bank 2 | ECM | DTC P0341, P0346, P0366, or P0391 for the 3.6L (LY7) engine DTC P0340, P0341, P0345, P0346, P0365, P0366, P0390, or P0391 for the 4.6L (LH2) engine
P0347 | Intake Camshaft Position (CMP) Sensor Circuit Low Voltage Bank 2 | ECM | DTC P0342, P0347, P0367, or P0392 for the 3.6L (LY7) engine
P0348 | Intake Camshaft Position (CMP) Sensor Circuit High Voltage Bank 2 | ECM | DTC P0343, P0348, P0368, or P0393 for the 3.6L (LY7) engine
P0351 | Ignition Coil 1 Control Circuit | ECM | DTC P0351-P0356 for the 3.6L (LY7) engine DTC P0351-P0358 for the 4.6L (LH2) engine
P0352 | Ignition Coil 2 Control Circuit | ECM | DTC P0351-P0356 for the 3.6L (LY7) engine DTC P0351-P0358 for the 4.6L (LH2) engine
P0353 | Ignition Coil 3 Control Circuit | ECM | DTC P0351-P0356 for the 3.6L (LY7) engine DTC P0351-P0358 for the 4.6L (LH2) engine
P0354 | Ignition Coil 4 Control Circuit | ECM | DTC P0351-P0356 for the 3.6L (LY7) engine DTC P0351-P0358 for the 4.6L (LH2) engine
P0355 | Ignition Coil 5 Control Circuit | ECM | DTC P0351-P0356 for the 3.6L (LY7) engine DTC P0351-P0358 for the 4.6L (LH2) engine
P0356 | Ignition Coil 6 Control Circuit | ECM | DTC P0351-P0356 for the 3.6L (LY7) engine DTC P0351-P0358 for the 4.6L (LH2) engine
P0357 | Ignition Coil 7 Control Circuit | ECM | DTC P0351-P0358 for the 4.6L (LH2) engine
P0358 | Ignition Coil 8 Control Circuit | ECM | DTC P0351-P0358 for the 4.6L (LH2) engine
P0365 | Exhaust Camshaft Position (CMP) Sensor Circuit Bank 1 | ECM | DTC P0340, P0341, P0345, P0346, P0365, P0366, P0390, or P0391 for the 4.6L (LH2) engine
P0366 | Exhaust Camshaft Position (CMP) Sensor Performance Bank 1 | ECM | DTC P0341, P0346, P0366, or P0391 for the 3.6L (LY7) engine DTC P0340, P0341, P0345, P0346, P0365, P0366, P0390, or P0391 for the 4.6L (LH2) engine
P0367 | Exhaust Camshaft Position (CMP) Sensor Circuit Low Voltage Bank 1 | ECM | DTC P0342, P0347, P0367, or P0392 for the 3.6L (LY7) engine
P0368 | Exhaust Camshaft Position (CMP) Sensor Circuit High Voltage Bank 1 | ECM | DTC P0343, P0348, P0368, or P0393 for the 3.6L (LY7) engine
P0390 | Exhaust Camshaft Position (CMP) Sensor Circuit Bank 2 | ECM | DTC P0340, P0341, P0345, P0346, P0365, P0366, P0390, or P0391 for the 4.6L (LH2) engine
P0391 | Exhaust Camshaft Position (CMP) Sensor Performance Bank 2 | ECM | DTC P0341, P0346, P0366, or P0391 for the 3.6L (LY7) engine DTC P0340, P0341, P0345, P0346, P0365, P0366, P0390, or P0391 for the 4.6L (LH2) engine
P0392 | Exhaust Camshaft Position (CMP) Sensor Circuit Low Voltage Bank 2 | ECM | DTC P0342, P0347, P0367, or P0392 for the 3.6L (LY7) engine
P0393 | Exhaust Camshaft Position (CMP) Sensor Circuit High Voltage Bank 2 | ECM | DTC P0343, P0348, P0368, or P0393 for the 3.6L (LY7) engine
P0420 | Catalyst System Low Efficiency Bank 1 | ECM | DTC P0420 or P0430 for the 3.6L (LY7) engine
Catalyst System Low Efficiency Bank 1 | ECM | DTC P0420 or P0430 for the 4.6L (LH2) engine
P0430 | Catalyst System Low Efficiency Bank 2 | ECM | DTC P0420 or P0430 for the 3.6L (LY7) engine
Catalyst System Low Efficiency Bank 2 | ECM | DTC P0420 or P0430 for the 4.6L (LH2) engine
P0443 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit | ECM | DTC P0443 for the 3.6L (LY7) engine DTC P0443 for the 4.6L (LH2) engine
P0458 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit Low Voltage | ECM | DTC P0458 for the 3.6L (LY7) engine
P0459 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit High Voltage | ECM | DTC P0459 for the 3.6L (LY7) engine
P0461 | Fuel Level Sensor 1 Performance | ECM | DTC P0461 for the 4.6L (LH2) engine
P0462 | Fuel Level Sensor 1 Circuit Low Voltage | ECM | DTC P0462 for the 4.6L (LH2) engine
P0463 | Fuel Level Sensor Circuit High Voltage | ECM | DTC P0463 for the 4.6L (LH2) engine
P0464 | Fuel Level Sensor Circuit Intermittent Failure | ECM | DTC P0464 for the 4.6L (LH2) engine
P0480 | Cooling Fan Relay 1 Control Circuit | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694 for the 3.6L (LY7) engine DTC P0480 or P0481 for the 4.6L (LH2) engine
P0481 | Cooling Fan Relay 2 Control Circuit | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694 for the 3.6L (LY7) engine DTC P0480 or P0481 for the 4.6L (LH2) engine
P0506 | Idle Speed Low | ECM | DTC P0506, P0507, or P050A for the 3.6L (LY7) engine DTC P0506 or P0507 for the 4.6L (LH2) engine
P0507 | Idle Speed High | ECM | DTC P0506, P0507, or P050A for the 3.6L (LY7) engine DTC P0506 or P0507 for the 4.6L (LH2) engine
P050A | Cold Start Idle Air Control (IAC) System Performance | ECM | DTC P0506, P0507, or P050A for the 3.6L (LY7) engine
P0521 | Engine Oil Pressure (EOP) Sensor Performance | ECM | DTC P0521 for the 3.6L (LY7) engine
P0522 | Engine Oil Pressure (EOP) Sensor Low Performance | ECM | DTC P0522
P0523 | Engine Oil Pressure (EOP) Sensor Circuit High Voltage | ECM | DTC P0523
P0532 | Air Conditioning (A/C) Refrigerant Pressure Sensor Circuit Low Voltage | ECM | DTC P0532 or P0533
P0533 | Air Conditioning (A/C) Refrigerant Pressure Sensor Circuit High Voltage | ECM | DTC P0532 or P0533
P0560 | Battery Voltage | ECM | DTC P0560 for the 3.6L (LY7) engine
P0562 | System Voltage Low | ECM | DTC P0562 for the 3.6L (LY7) engine
TCM | DTC P0562 or P0563 for the 6L50-E transmission
P0563 | System Voltage High | ECM | DTC P0563
TCM | DTC P0562 or P0563 for the 6L50-E transmission
P0571 | Brake Switch Circuit 1 | ECM | DTC P0571 for the 3.6L (LY7) engine
P0572 | Brake Switch Circuit 1 Low Voltage | ECM | DTC P0572 for the 4.6L (LH2) engine
P0573 | Brake Switch Circuit 1 High Voltage | ECM | DTC P0573 for the 4.6L (LH2) engine
P0575 | Cruise Control Switch Signal Circuit | ECM | DTC P0575
P0601 | Control Module Read Only Memory (ROM) | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 3.6L (LY7) engine DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610 for the 4.6L (LH2) engine
Transmission Control Module (TCM) Read Only Memory (ROM) | TCM | DTC P0601-P0604 or P062F for the 5L40-E transmission DTC P0601-P0604 or P062F for the 6L50-E transmission
P0602 | Control Module Not Programmed | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 3.6L (LY7) engine DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610 for the 4.6L (LH2) engine
Transmission Control Module (TCM) Not Programmed | TCM | DTC P0601-P0604 or P062F for the 5L40-E transmission DTC P0601-P0604 or P062F for the 6L50-E transmission
P0603 | Control Module (TCM) Long Term Memory Reset | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 3.6L (LY7) engine DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610 for the 4.6L (LH2) engine
Transmission Control Module (TCM) Long Term Memory Reset | TCM | DTC P0601-P0604 or P062F for the 5L40-E transmission DTC P0601-P0604 or P062F for the 6L50-E transmission
P0604 | Control Module Random Access Memory (RAM) | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 3.6L (LY7) engine DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610 for the 4.6L (LH2) engine
Transmission Control Module (TCM) Random Access Memory (RAM) | TCM | DTC P0601-P0604 or P062F for the 5L40-E transmission DTC P0601-P0604 or P062F for the 6L50-E transmission
P0606 | Control Module Performance | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 3.6L (LY7) engine DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610 for the 4.6L (LH2) engine
P0607 | Control Module Internal Performance | ECM | DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610 for the 4.6L (LH2) engine
P0608 | Vehicle Speed Output Circuit | ECM | DTC P0608
P060D | Control Module Accelerator Pedal Position (APP) System Performance | ECM | DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610 for the 4.6L (LH2) engine
P0615 | Starter Relay Control Circuit | ECM | DTC P0615
P0616 | Starter Relay Control Circuit Low Voltage | ECM | DTC P0616 for the 3.6L (LY7) engine
P0617 | Starter Relay Control Circuit High Voltage | ECM | DTC P0617 for the 3.6L (LY7) engine
P0621 | Generator L Terminal Circuit | ECM | DTC P0621
P0622 | Generator F Terminal Circuit | ECM | DTC P0622 for the 4.6L (LH2) engine
P0625 | Generator F-Terminal Circuit Low Voltage | ECM | DTC P0625 for the 3.6L (LY7) engine
P0626 | Generator F-Terminal Circuit High Voltage | ECM | DTC P0626 for the 3.6L (LY7) engine
P0627 | Fuel Pump Relay Control Circuit | ECM | DTC P0627 for the 3.6L (LY7) engine
P0628 | Fuel Pump Relay Control Circuit Low Voltage | ECM | DTC P0628 for the 3.6L (LY7) engine
P0629 | Fuel Pump Relay Control Circuit High Voltage | ECM | DTC P0629 for the 3.6L (LY7) engine
P062F | Control Module (TCM) Long Term Memory Performance | ECM | DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610 for the 4.6L (LH2) engine
Transmission Control Module (TCM) Long Term Memory Performance | TCM | DTC P0601-P0604 or P062F for the 5L40-E transmission DTC P0601-P0604 or P062F for the 6L50-E transmission
P0634 | Transmission Control Module (TCM) Overtemperature | TCM | DTC P0634 for the 6L50-E transmission
P0638 | Throttle Actuator Control (TAC) Command Performance | ECM | DTC P0638 for the 3.6L (LY7) engine
P0641 | 5V Reference 1 Circuit | ECM | DTC P0641-P0643 for the 3.6L (LY7) engine
5V Reference Voltage 1 Circuit | DTC P0641 or P0651 for the 4.6L (LH2) engine
P0642 | 5V Reference Voltage 1 Circuit Low Voltage | ECM | DTC P0641-P0643
P0643 | 5V Reference Voltage 1 Circuit High Voltage | ECM | DTC P0641-P0643
P0645 | Air Conditioning (A/C) Clutch Relay Control Circuit | ECM | DTC P0645, P0646, or P0647 or DTC P0645
P0646 | Air Conditioning (A/C) Clutch Relay Control Circuit Low Voltage | ECM | DTC P0645, P0646, or P0647
P0647 | Air Conditioning (A/C) Clutch Relay Control Circuit High Voltage | ECM | DTC P0645, P0646, or P0647
P0650 | Malfunction Indicator Lamp (MIL) Control Circuit | ECM | DTC P0650 for the 3.6L (LY7) engine DTC P0650 for the 4.6L (LH2) engine
P0651 | 5V Reference 2 Circuit | ECM | DTC P0651 - P0653 for the 3.6L (LY7) engine
5V Reference Voltage 2 Circuit | DTC P0641 or P0651 for the 4.6L (LH2) engine
P0652 | 5V Reference Voltage 2 Circuit Low Voltage | ECM | DTC P0651 - P0653 for the 3.6L (LY7) engine
P0653 | 5V Reference Voltage 2 Circuit High Voltage | ECM | DTC P0660 - P0653 for the 3.6L (LY7) engine
P0660 | Variable Intake manifold Tuning (IMT) Solenoid Control Circuit | ECM | DTC P0660 or P2008 for the 3.6L (LY7) engine
P0661 | Variable Intake manifold Tuning (IMT) Solenoid Control Circuit | ECM | DTC P0661 or P2009 for the 3.6L (LY7) engine
P0662 | Variable Intake manifold Tuning (IMT) Solenoid Control Circuit | ECM | DTC P0662 or P2010 for the 3.6L (LY7) engine
P0667 | Transmission Control Module (TCM) Temperature Sensor Performance | TCM | DTC P0667, P0668, or P0669 for the 6L50-E transmission
P0668 | Transmission Control Module (TCM) Temperature Sensor Circuit High Voltage | TCM | DTC P0667, P0668, or P0669 for the 6L50-E transmission
P0669 | Transmission Control Module (TCM) Temperature Sensor Circuit Low Voltage | TCM | DTC P0667, P0668, or P0669 for the 6L50-E transmission
P0685 | Engine Control System Ignition Relay Control Circuit | ECM | DTC P0685, P0686, P0687, P0689, or P0690 for the 3.6L (LY7) engine DTC P0685 or P0690 for the 4.6L (LH2) engine
P0686 | Engine Control System Ignition Relay Control Circuit Low Voltage | ECM | DTC P0685, P0686, P0687, P0689, or P0690 for the 3.6L (LY7) engine
P0687 | Engine Control System Ignition Relay Control Circuit High Voltage | ECM | DTC P0685, P0686, P0687, P0689, or P0690 for the 3.6L (LY7) engine
P0689 | Engine Control System Ignition Relay Feedback Circuit Low Voltage | ECM | DTC P0685, P0686, P0687, P0689, or P0690 for the 3.6L (LY7) engine
P0690 | Engine Control System Ignition Relay Feedback Circuit High Voltage | ECM | DTC P0685, P0686, P0687, P0689, or P0690 for the 3.6L (LY7) engine DTC P0685 or P0690 for the 4.6L (LH2) engine
P0691 | Cooling Fan Relay 1 Control Circuit Low Voltage | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694 for the 3.6L (LY7) engine
P0692 | Cooling Fan Relay 1 Control Circuit High Voltage | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694 for the 3.6L (LY7) engine
P0693 | Cooling Fan Relay 2 Control Circuit Low Voltage | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694 for the 3.6L (LY7) engine
P0694 | Cooling Fan Relay 2 Control Circuit High Voltage | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694 for the 3.6L (LY7) engine
P0697 | 5V Reference 3 Circuit | ECM | DTC P0697-P0699 for the 3.6L (LY7) engine
P0698 | 5V Reference Voltage 3 Circuit Low Voltage | ECM | DTC P0697-P0699 for the 3.6L (LY7) engine
P0699 | 5V Reference Voltage 3 Circuit High Voltage | ECM | DTC P0697-P0699 for the 3.6L (LY7) engine
P0700 | Transmission Control Module (TCM) Requested MIL Illumination | ECM | DTC P0700 for the 3.6L (LY7) engine DTC P0700 for the 4.6L (LH2) engine
P0703 | Brake Switch Circuit 2 | TCM | DTC P0703 for the 4.6L (LH2) engine
P0711 | Transmission Fluid Temperature (TFT) Sensor Performance | TCM | DTC P0711 for the 5L40-E transmission DTC P0711, P0712, or P0713 for the 6L50-E transmission
P0712 | Transmission Fluid Temperature (TFT) Sensor Circuit Low Voltage | TCM | DTC P0712 for the 5L40-E transmission DTC P0711, P0712, or P0713 for the 6L50-E transmission
P0713 | Transmission Fluid Temperature (TFT) Sensor Circuit High Voltage | TCM | DTC P0713 for the 5L40-E transmission DTC P0711, P0712, or P0713 for the 6L50-E transmission
P0716 | Input Speed Sensor Performance | TCM | DTC P0716 for the 5L40-E transmission DTC P0716 or P0717 for the 6L50-E transmission
P0717 | Input Speed Sensor Circuit Low Voltage | TCM | DTC P0717 for the 5L40-E transmission DTC P0716 or P0717 for the 6L50-E transmission
P0719 | Brake Switch Circuit Low Input | TCM | DTC P0719 for the 6L50-E transmission
P0722 | Input Speed Sensor Circuit Low Voltage | TCM | DTC P0722 for the 5L40-E transmission DTC P0722 or P0723 for the 6L50-E transmission
P0723 | Output Speed Sensor Circuit Intermittent | TCM | DTC P0723 for the 5L40-E transmission DTC P0722 or P0723 for the 6L50-E transmission
P0724 | Brake Switch Circuit High Input | TCM | DTC P0724 for the 6L50-E transmission
P0727 | Engine Speed No Signal | TCM | DTC P0727 for the 5L40-E transmission
P0741 | Torque Converter Clutch (TCC) System - Stuck Off | TCM | DTC P0741 for the 5L40-E transmission DTC P0741 or P0742 for the 6L50-E transmission
P0742 | Torque Converter Clutch (TCC) System - Stuck On | TCM | DTC P0742 for the 5L40-E transmission DTC P0741 or P0742 for the 6L50-E transmission
P0751 | 1-2 Shift Solenoid (SS) Valve Performance - No First, Fourth or Fifth Gear | TCM | DTC P0751 for the 5L40-E transmission DTC P0751 for the 6L50-E transmission
P0752 | 1-2 Shift Solenoid (SS) Valve Performance - No Second or Third Gear | TCM | DTC P0752 for the 5L40-E transmission DTC P0752 for the 6L50-E transmission
P0756 | Shift Solenoid (SS) Valve Performance - No First or Second Gear | TCM | DTC P0756 for the 5L40-E transmission DTC P0756 for the 6L50-E transmission
P0757 | 2-3 Shift Solenoid (SS) Valve Performance - No Third, Fourth or Fifth Gear | TCM | DTC P0757 for the 5L40-E transmission
P0761 | 4-5 Shift Solenoid (SS) Valve Performance - No Fourth Gear | TCM | DTC P0761 for the 5L40-E transmission
P0762 | 4-5 Shift Solenoid (SS) Valve Performance - No Fourth Gear | TCM | DTC P0762 for the 5L40-E transmission
P0776 | Clutch Pressure Control (PC) Solenoid Valve 2 - Stuck Off | TCM | DTC P0776 or P0777 for the 6L50-E transmission
P0777 | Clutch Pressure Control (PC) Solenoid Valve 2 - Stuck On | TCM | DTC P0776 or P0777 for the 6L50-E transmission
P0796 | Clutch Pressure Control (PC) Solenoid Valve 3 - Stuck Off | TCM | DTC P0796 or P0797 for the 6L50-E transmission
P0797 | Clutch Pressure Control (PC) Solenoid Valve 3 - Stuck On | TCM | DTC P0796 or P0797 for the 6L50-E transmission
P0815 | Upshift Switch Circuit | TCM | DTC P0815 for the 5L40-E transmission DTC P0815, P0816, P0826, or P1876 for the 6L50-E transmission
P0816 | Downshift Switch Circuit | TCM | DTC P0816 for the 5L40-E transmission DTC P0815, P0816, P0826, or P1876 for the 6L50-E transmission
P0826 | Up and Down Shift Switch Circuit | TCM | DTC P0826 for the 5L40-E transmission DTC P0815, P0816, P0826, or P1876 for the 6L50-E transmission
P0842 | Transmission Fuel Pressure (TFP) Switch 1 Circuit Low Voltage | TCM | DTC P0842 or P0843 for the 6L50-E transmission
P0843 | Transmission Fuel Pressure (TFP) Switch 1 Circuit High Voltage | TCM | DTC P0842 or P0843 for the 6L50-E transmission
P0850 | Park/Neutral Position (PNP) Switch Circuit | ECM | DTC P0850 for the 3.6L (LY7) engine
P0851 | Park/Neutral Position (PNP) Switch Circuit Low Voltage | ECM | DTC P0851 or P0852 for the 4.6L (LH2) engine
P0852 | Park/Neutral Position (PNP) Switch Circuit High Voltage | ECM | DTC P0851 or P0852 for the 4.6L (LH2) engine
P0856 | Traction Control System Input Signal | ECM | DTC P0856
P0872 | Transmission Fuel Pressure (TFP) Switch 3 Circuit Low Voltage | TCM | DTC P0872 or P0873 for the 6L50-E transmission
P0873 | Transmission Fuel Pressure (TFP) Switch 3 Circuit High Voltage | TCM | DTC P0872 or P0873 for the 6L50-E transmission
P0877 | Transmission Fuel Pressure (TFP) Switch 4 Circuit Low Voltage | TCM | DTC P0877 or P0878 for the 6L50-E transmission
P0878 | Transmission Fuel Pressure (TFP) Switch 4 Circuit High Voltage | TCM | DTC P0877 or P0878 for the 6L50-E transmission
P0961 | Pipeline Pressure Control (PC) Solenoid Valve System Performance | TCM | DTC P0961-P0963 for the 6L50-E transmission
P0962 | Pipeline Pressure Control (PC) Solenoid Valve Control Circuit Low Voltage | TCM | DTC P0961-P0963 for the 6L50-E transmission
P0963 | Pipeline Pressure Control (PC) Solenoid Valve Control Circuit High Voltage | TCM | DTC P0961-P0963 for the 6L50-E transmission
P0965 | Clutch Pressure Control (PC) Solenoid Valve System Performance | TCM | DTC P0965-P0967 for the 6L50-E transmission
P0966 | Pipeline Pressure Control (PC) Solenoid Valve 2 Control Circuit Low Voltage | TCM | DTC P0965-P0967 for the 6L50-E transmission
P0967 | Pipeline Pressure Control (PC) Solenoid Valve 2 Control Circuit High Voltage | TCM | DTC P0965-P0967 for the 6L50-E transmission
P0969 | Clutch Pressure Control (PC) Solenoid Valve 3 System Performance | TCM | DTC P0969-P0971 for the 6L50-E transmission
P0970 | Pipeline Pressure Control (PC) Solenoid Valve 3 Control Circuit Low Voltage | TCM | DTC P0969-P0971 for the 6L50-E transmission
P0971 | Pipeline Pressure Control (PC) Solenoid Valve 3 Control Circuit High Voltage | TCM | DTC P0969-P0971 for the 6L50-E transmission
P0973 | 1-2 Shift Solenoid (SS) Control Circuit Low Voltage | TCM | DTC P0973 for the 5L40-E transmission
Shift Solenoid (SS) 1 Control Circuit Low Voltage | TCM | DTC P0973 or P0974 for the 6L50-E transmission
P0974 | 1-2 Shift Solenoid (SS) Control Circuit High Voltage | TCM | DTC P0974 for the 5L40-E transmission
Shift Solenoid (SS) 1 Control Circuit High Voltage | TCM | DTC P0973 or P0974 for the 6L50-E transmission
P0976 | 2-3 Shift Solenoid (SS) Control Circuit Low Voltage | TCM | DTC P0976 for the 5L40-E transmission
Shift Solenoid (SS) 2 Control Circuit Low Voltage | TCM | DTC P0976 or P0977 for the 6L50-E transmission
P0977 | 2-3 Shift Solenoid (SS) Control Circuit High Voltage | TCM | DTC P0977 for the 5L40-E transmission
Shift Solenoid (SS) 2 ontrol Circuit High Voltage | TCM | DTC P0976 or P0977 for the 6L50-E transmission
P0979 | 4-5 Shift Solenoid (SS) Control Circuit Low Voltage | TCM | DTC P0979 for the 5L40-E transmission
P0980 | 4-5 Shift Solenoid (SS) Control Circuit High Voltage | TCM | DTC P0980 for the 5L40-E transmission
P0989 | Transmission Fuel Pressure (TFP) Switch 5 Circuit Low Voltage | TCM | DTC P0989 or P0990 for the 6L50-E transmission
P0990 | Transmission Fuel Pressure (TFP) Switch 5 Circuit High Voltage | TCM | DTC P0989 or P0990 for the 6L50-E transmission
P1011 | Intake Camshaft Position (CMP) Actuator Park Position Bank 1 | ECM | DTC P1011-P1014 for the 3.6L (LY7) engine
P1012 | Exhaust Camshaft Position (CMP) Actuator Park Position Bank 1 | ECM | DTC P1011-P1014 for the 3.6L (LY7) engine
P1013 | Intake Camshaft Position (CMP) Actuator Park Position Bank 2 | ECM | DTC P1011-P1014 for the 3.6L (LY7) engine
P1014 | Exhaust Camshaft Position (CMP) Actuator Park Position Bank 2 | ECM | DTC P1011-P1014 for the 3.6L (LY7) engine
P1101 | Intake Air Flow System Performance | ECM | DTC P0101 or P1101 for the 4.6L (LH2) engine
P1133 | HO2S Insufficient Convert Bank 1 Sensor 1 | ECM | DTC P0133, P0134, P0140, P1133, or P2A00 for the 4.6L (LH2) engine
P1153 | HO2S Insufficient Convert Bank 2 Sensor 1 | ECM | DTC P0153,P0154, P0160, P1153, or P2A03 for the 4.6L (LH2) engine
P1258 | Engine Coolant Overtemperature - Protection Mode Active | ECM | DTC P1258 (3.6L (LY7)) in Engine Electrical DTC P1258
P1380 | Misfire Detected - Rough Road Data Not Available | ECM | DTC P1380 for the 3.6L (LY7) engine DTC P1380 or P1381 for the 4.6L (LH2) engine
P1381 | Misfire Detected - No Communication With Brake Control Module | ECM | DTC P1380 or P1381
P1400 | Cold Start Emission Reduction Control System | ECM | DTC P1400 for the 4.6L (LH2) engine
P1516 | Throttle Actuator Control (TAC) Module Throttle Actuator Position Performance | ECM | DTC P1516, P2101, P2119, or P2176 for the 4.6L (LH2) engine
P1551 | Throttle Valve Rest Position Not Reached During Learn | ECM | DTC P1551 for the 3.6L (LY7) engine
P1629 | Theft Deterrent Fuel Enable Signal Not Recieved | ECM | DTC P1629
P1630 | Theft Deterrent Learn Mode Active | ECM | DTC P1630
P1631 | Theft Deterrent Fuel Enable Signal Not Correct | ECM | DTC P1631
P167A | Control Module HO2S Bank 1 Sensor 1 System Performance | ECM | DTC P167A for the 3.6L (LY7) engine
P167B | Control Module HO2S Bank 2 Sensor 1 System Performance | ECM | DTC P167B for the 3.6L (LY7) engine
P1682 | Ignition 1 Switch Circuit 2 | ECM | DTC P1682 for the 4.6L (LH2) engine
P1684 | Transmission Control Module (TCM) Power on Temperature Sensor Performance | TCM | DTC P1684-P1686 for the 6L50-E transmission
P1685 | Transmission Control Module (TCM) Power on Temperature Sensor Circuit Low Voltage | TCM | DTC P1684-P1686 for the 6L50-E transmission
P1686 | Transmission Control Module (TCM) Power on Temperature Sensor Circuit High Voltage | TCM | DTC P1684-P1686 for the 6L50-E transmission
P1751 | Shift Valve 1 Performance | TCM | DTC P1751 for the 6L50-E transmission
P1820 | Internal Mode Switch A Circuit Low Voltage | TCM | DTC P1820 for the 5L40-E transmission
P1822 | Internal Mode Switch B Circuit High Voltage | TCM | DTC P1822 for the 5L40-E transmission
P1823 | Internal Mode Switch P Circuit Low Voltage | TCM | DTC P1823 for the 5L40-E transmission
P1825 | Internal Mode Switch - Invalid Range | TCM | DTC P1825 for the 5L40-E transmission DTC P1825 or P1915 for the 6L50-E transmission
P1826 | Internal Mode Switch C Circuit High Voltage | TCM | DTC P1826 for the 5L40-E transmission
P1831 | Pressure Control (PC)/Shift Lock Solenoid Control Circuit Low Voltage | TCM | DTC P1831 or P1832 for the 6L50-E transmission
P1832 | Pressure Control (PC)/Shift Lock Solenoid Control Circuit High Voltage | TCM | DTC P1831 or P1832 for the 6L50-E transmission
P1833 | Torque Converter Clutch (TCC)/Shift Solenoid (SS) Control Circuit Low Voltage | TCM | DTC P1833 for the 5L40-E transmission
P1834 | Torque Converter Clutch (TCC)/Shift Solenoid (SS) Control Circuit High Voltage | TCM | DTC P1834 for the 5L40-E transmission
P1876 | Up and Down Shift Switch Performance-Range Switch Not in D3 | TCM | DTC P1876 for the 5L40-E transmission DTC P0815, P0816, P0826, or P1876 for the 6L50-E transmission
P1915 | Internal Mode Switch Not Command Park/Neutral During Starting Procedure | TCM | DTC P1915 for the 5L40-E transmission
Internal Mode Switch - Start/Invalid Range | TCM | DTC P1825 or P1915 for the 6L50-E transmission
P2008 | Intake Manifold Runner Control (IMRC) Solenoid Control Circuit | ECM | DTC P2008 for the 3.6L (LY7) engine
P2009 | Intake Manifold Runner Control (IMRC) Solenoid Control Circuit Low Voltage | ECM | DTC P2009 for the 3.6L (LY7) engine
P2010 | Intake Manifold Runner Control (IMRC) Solenoid Control Circuit High Voltage | ECM | DTC P2010 for the 3.6L (LY7) engine
P2066 | Fuel Level Sensor 2 Performance | ECM | DTC P2066
P2067 | Fuel Level Sensor 2 Circuit Low Voltage | ECM | DTC P2067
P2068 | Fuel Level Sensor 2 Circuit High Voltage | ECM | DTC P2068
P2088 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit Low Voltage Bank 1 | ECM | DTC P2088, P2090, P2092, or P2094 for the 3.6L (LY7) engine
P2089 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit High Voltage Bank 1 | ECM | DTC P2089, P2091, P2093, or P2095 for the 3.6L (LY7) engine
P2090 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit Low Voltage Bank 1 | ECM | DTC P2088, P2090, P2092, or P2094 for the 3.6L (LY7) engine
P2091 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit High Voltage Bank 1 | ECM | DTC P2089, P2091, P2093, or P2095 for the 3.6L (LY7) engine
P2092 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit Low Voltage Bank 2 | ECM | DTC P2088, P2090, P2092, or P2094 for the 3.6L (LY7) engine
P2093 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit High Voltage Bank 2 | ECM | DTC P2089, P2091, P2093, or P2095 for the 3.6L (LY7) engine
P2094 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit Low Voltage Bank 2 | ECM | DTC P2088, P2090, P2092, or P2094 for the 3.6L (LY7) engine
P2095 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit High Voltage Bank 2 | ECM | DTC P2089, P2091, P2093, or P2095 for the 3.6L (LY7) engine
P2096 | Post Catalyst Fuel Trim System Low Limit Bank 1 | ECM | DTC P2096 or P2098 for the 3.6L (LY7) engine
P2097 | Post Catalyst Fuel Trim System High Limit Bank 1 | ECM | DTC P2097 or P2099 for the 3.6L (LY7) engine
P2098 | Post Catalyst Fuel Trim System Low Limit Bank 2 | ECM | DTC P2096 or P2098 for the 3.6L (LY7) engine
P2099 | Post Catalyst Fuel Trim System High Limit Bank 2 | ECM | DTC P2097 or P2099 for the 3.6L (LY7) engine
P2100 | Throttle Actuator Control (TAC) Motor Control Circuit | ECM | DTC P2100 for the 3.6L (LY7) engine
P2101 | Control Module Throttle Actuator Position Performance | ECM | DTC P2101 for the 3.6L (LY7) engine
Throttle Actuator Position Performance | ECM | DTC P1516, P2101, P2119, or P2176 for the 4.6L (LH2) engine
P2105 | Throttle Actuator Control (TAC) System - Forced Engine Shutdown | ECM | DTC P2105 for the 3.6L (LY7) engine
P2107 | Throttle Actuator Control (TAC) Module Internal Circuit | ECM | DTC P2107 for the 3.6L (LY7) engine
P2119 | Throttle Closed Position Performance | ECM | DTC P2119 for the 3.6L (LY7) engine DTC P1516, P2101, P2119, or P2176 for the 4.6L (LH2) engine
P2120 | Accelerator Pedal Position (APP) Sensor 1 Circuit | ECM | DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 4.6L (LH2) engine
P2122 | Accelerator Pedal Position (APP) Sensor 1 Circuit Low Voltage | ECM | DTC P2122 for the 3.6L (LY7) engine DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 4.6L (LH2) engine
P2123 | Accelerator Pedal Position (APP) Sensor 1 Circuit High Voltage | ECM | DTC P2123 for the 3.6L (LY7) engine DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 4.6L (LH2) engine
P2125 | Accelerator Pedal Position (APP) Sensor 2 Circuit | ECM | DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 4.6L (LH2) engine
P2127 | Accelerator Pedal Position (APP) Sensor 2 Circuit Low Voltage | ECM | DTC P2127 for the 3.6L (LY7) engine DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 4.6L (LH2) engine
P2128 | Accelerator Pedal Position (APP) Sensor 2 Circuit High Voltage | ECM | DTC P2128 for the 3.6L (LY7) engine DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 4.6L (LH2) engine
P2135 | Throttle Position (TP) Sensor 1-2 Correlation | ECM | DTC P0120, P0122, P0123, P0220, P0222, P0223, or P2135 for the 4.6L (LH2) engine
P2138 | Accelerator Pedal Position (APP) Sensor 1-2 Correlation | ECM | DTC P2138 for the 3.6L (LY7) engine DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 4.6L (LH2) engine
P2176 | Minimum Throttle Position Not Learned | ECM | DTC P2176 for the 3.6L (LY7) engine DTC P1516, P2101, P2119, or P2176 for the 4.6L (LH2) engine
P2177 | Fuel Trim System Lean at Cruise or Accel Bank 1 | ECM | DTC P2177 or P2179 for the 3.6L (LY7) engine
P2178 | Fuel Trim System Rich at Cruise or Accel Bank 1 | ECM | DTC P2178 or P2180 for the 3.6L (LY7) engine
P2179 | Fuel Trim System Lean at Cruise or Accel Bank 2 | ECM | DTC P2177 or P2179 for the 3.6L (LY7) engine
P2180 | Fuel Trim System Rich at Cruise or Accel Bank 2 | ECM | DTC P2178 or P2180 for the 3.6L (LY7) engine
P2187 | Fuel Trim System Lean at Idle Bank 1 | ECM | DTC P2187 or P2189 for the 3.6L (LY7) engine
P2188 | Fuel Trim System Rich at Idle Bank 1 | ECM | DTC P2188 or P2190 for the 3.6L (LY7) engine
P2189 | Fuel Trim System Lean at Idle Bank 2 | ECM | DTC P2187 or P2189 for the 3.6L (LY7) engine
P2190 | Fuel Trim System Rich at Idle Bank 2 | ECM | DTC P2188 or P2190 for the 3.6L (LY7) engine
P2195 | HO2S Signal Biased Lean Bank 1 Sensor 1 | ECM | DTC P2195 or P2197 for the 3.6L (LY7) engine
P2196 | HO2S Signal Biased Rich Bank 1 Sensor 1 | ECM | DTC P2196 or P2198 for the 3.6L (LY7) engine
P2197 | HO2S Signal Biased Lean BanK 2 Sensor 1 | ECM | DTC P2195 or P2197 for the 3.6L (LY7) engine
P2198 | HO2S Signal Biased Rich Bank 2 Sensor 1 | ECM | DTC P2196 or P2198 for the 3.6L (LY7) engine
P2227 | Barometric Pressure (BARO) Sensor Performance | ECM | DTC P2227 for the 3.6L (LY7) engine
P2228 | Barometric Pressure (BARO) Sensor Circuit Low Voltage | ECM | DTC P2228 for the 3.6L (LY7) engine
P2229 | Barometric Pressure (BARO) Sensor Circuit High Voltage | ECM | DTC P2229 for the 3.6L (LY7) engine
P2231 | HO2S Signal Circuit Shorted to Heater Circuit Bank 1 Sensor 1 | ECM | DTC P2231 or P2234 for the 3.6L (LY7) engine
P2232 | HO2S Signal Circuit Shorted to Heater Circuit Bank 1 Sensor 2 | ECM | DTC P2232 or P2235 for the 3.6L (LY7) engine
P2234 | HO2S Signal Circuit Shorted to Heater Circuit Bank 2 Sensor 1 | ECM | DTC P2231 or P2234 for the 3.6L (LY7) engine
P2235 | HO2S Signal Circuit Shorted to Heater Circuit Bank 2 Sensor 2 | ECM | DTC P2232 or P2235 for the 3.6L (LY7) engine
P2237 | HO2S Pumping Current Control Circuit Bank 1 Sensor 1 | ECM | DTC P2237 or P2240 for the 3.6L (LY7) engine
P2240 | HO2S Pumping Current Control Circuit Bank 2 Sensor 1 | ECM | DTC P2237 or P2240 for the 3.6L (LY7) engine
P2243 | HO2S Reference Voltage Circuit Bank 1 Sensor 1 | ECM | DTC P2243 or P2247 for the 3.6L (LY7) engine
P2247 | HO2S Reference Voltage Circuit Bank 2 Sensor 1 | ECM | DTC P2243 or P2247 for the 3.6L (LY7) engine
P2251 | HO2S Low Reference Circuit Bank 1 Sensor 1 | ECM | DTC P2251 or P2254 for the 3.6L (LY7) engine
P2254 | HO2S Low Reference Circuit Bank 2 Sensor 1 | ECM | DTC P2251 or P2254 for the 3.6L (LY7) engine
P2270 | HO2S Signal Stuck Lean Bank 1 Sensor 2 | ECM | DTC P2270 or P2272 for the 3.6L (LY7) engine
P2271 | HO2S Signal Stuck Rich Bank 1 Sensor 2 | ECM | DTC P2271 or P2273 for the 3.6L (LY7) engine
P2272 | HO2S Signal Stuck Lean Bank 2 Sensor 2 | ECM | DTC P2270 or P2272 for the 3.6L (LY7) engine
P2273 | HO2S Signal Stuck Rich Bank 2 Sensor 2 | ECM | DTC P2271 or P2273 for the 3.6L (LY7) engine
P2297 | HO2S Signal Stuck Lean Bank 2 Sensor 2 | ECM | DTC P2297 or P2298 for the 3.6L (LY7) engine
P2298 | HO2S Performance During Decel Fuel Cut-Off (DFCO) Bank 2 Sensor 1 | ECM | DTC P2297 or P2298 for the 3.6L (LY7) engine
P2300 | Ignition Coil 1 Control Circuit Low Voltage | ECM | DTC P2300, P2303, P2306, P2309, P2312, or P2315 for the 3.6L (LY7) engine
P2301 | Ignition Coil 1 Control Circuit High Voltage | ECM | DTC P2301, P2304, P2307, P2310, P2313, or P2316 for the 3.6L (LY7) engine
P2303 | Ignition Coil 2 Control Circuit Low Voltage | ECM | DTC P2300, P2303, P2306, P2309, P2312, or P2315 for the 3.6L (LY7) engine
P2304 | Ignition Coil 2 Control Circuit High Voltage | ECM | DTC P2301, P2304, P2307, P2310, P2313, or P2316 for the 3.6L (LY7) engine
P2306 | Ignition Coil 3 Control Circuit Low Voltage | ECM | DTC P2300, P2303, P2306, P2309, P2312, or P2315 for the 3.6L (LY7) engine
P2307 | Ignition Coil 3 Control Circuit High Voltage | ECM | DTC P2301, P2304, P2307, P2310, P2313, or P2316 for the 3.6L (LY7) engine
P2309 | Ignition Coil 4 Control Circuit Low Voltage | ECM | DTC P2300, P2303, P2306, P2309, P2312, or P2315 for the 3.6L (LY7) engine
P2310 | Ignition Coil 4 Control Circuit High Voltage | ECM | DTC P2301, P2304, P2307, P2310, P2313, or P2316 for the 3.6L (LY7) engine
P2312 | Ignition Coil 5 Control Circuit Low Voltage | ECM | DTC P2300, P2303, P2306, P2309, P2312, or P2315 for the 3.6L (LY7) engine
P2313 | Ignition Coil 5 Control Circuit High Voltage | ECM | DTC P2301, P2304, P2307, P2310, P2313, or P2316 for the 3.6L (LY7) engine
P2315 | Ignition Coil 6 Control Circuit Low Voltage | ECM | DTC P2300, P2303, P2306, P2309, P2312, or P2315 for the 3.6L (LY7) engine
P2316 | Ignition Coil 6 Control Circuit High Voltage | ECM | DTC P2301, P2304, P2307, P2310, P2313, or P2316 for the 3.6L (LY7) engine
P2534 | Ignition 1 Switch Circuit Low Voltage | TCM | DTC P2534 for the 5L40-E transmission DTC P2534 for the 6L50-E transmission
P2544 | Transmission Torque Request Circuit | TCM | DTC P2544 for the 5L40-E transmission DTC P2544 for the 4.6L (LH2) engine
P2610 | Control Module Ignition Switch OFF Timer Performance | ECM | DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610 for the 4.6L (LH2) engine
P2626 | HO2S Pumping Current Trim Circuit Bank 1 Sensor 1 | ECM | DTC P2626 or P2629 for the 3.6L (LY7) engine
P2629 | HO2S Pumping Current Trim Circuit Bank 2 Sensor 1 | ECM | DTC P2626 or P2629 for the 3.6L (LY7) engine
P2636 | Fuel Transfer Pump Flow Insufficient | ECM | DTC P2636 for the 3.6L (LY7) engine
P2637 | Transmission Torque Delivered Circuit | TCM | DTC P2637 for the 5L40-E transmission
P2714 | Clutch Pressure Control (PC) Solenoid Valve 4 - Stuck OFF | TCM | DTC P2714 or P2715 for the 6L50-E transmission
P2715 | Clutch Pressure Control (PC) Solenoid Valve 4 - Stuck On | TCM | DTC P2714 or P2715 for the 6L50-E transmission
P2719 | Clutch Pressure Control (PC) Solenoid Valve 4 System Performance | TCM | DTC P2719-P2721 for the 6L50-E transmission
P2720 | Pipeline Pressure Control (PC) Solenoid Valve 4 Control Circuit Low Voltage | TCM | DTC P2719-P2721 for the 6L50-E transmission
P2721 | Pipeline Pressure Control (PC) Solenoid Valve 4 Control Circuit High Voltage | TCM | DTC P2719-P2721 for the 6L50-E transmission
P2723 | Clutch Pressure Control (PC) Solenoid Valve 5 - Stuck OFF | TCM | DTC P2723 or P2724 for the 6L50-E transmission
P2724 | Clutch Pressure Control (PC) Solenoid Valve 5 - Stuck On | TCM | DTC P2723 or P2724 for the 6L50-E transmission
P2728 | Clutch Pressure Control (PC) Solenoid Valve 5 System Performance | TCM | DTC P2728-P2730 for the 6L50-E transmission
P2729 | Pipeline Pressure Control (PC) Solenoid Valve 5 Control Circuit High Voltage | TCM | DTC P2728-P2730 for the 6L50-E transmission
P2730 | Pipeline Pressure Control (PC) Solenoid Valve 5 Control Circuit Low Voltage | TCM | DTC P2728-P2730 for the 6L50-E transmission
P2762 | Torque Converter Clutch (TCC) Pressure Control Solenoid Valve System Performance | TCM | DTC P2762, P2763, or P2764 for the 6L50-E transmission
P2763 | Torque Converter Clutch (TCC) Pressure Control (PC) Solenoid Valve Control Circuit High Voltage | TCM | DTC P2763 for the 5L40-E transmission
Torque Converter Clutch (TCC) Pressure Control (PC) Solenoid Valve Control Circuit Low Voltage | TCM | DTC P2762, P2763, or P2764 for the 6L50-E transmission
P2764 | Torque Converter Clutch (TCC) Pressure Control (PC) Solenoid Valve Control Circuit Low Voltage | TCM | DTC P2764 for the 5L40-E transmission
Torque Converter Clutch (TCC) Pressure Control (PC) Solenoid Valve Control Circuit High Voltage | TCM | DTC P2762, P2763, or P2764 for the 6L50-E transmission
P2A00 | HO2S Performance Bank 1 Sensor 1 | ECM | DTC P0133, P0134, P0140, P1133, or P2A00 for the 4.6L (LH2) engine
P2A01 | HO2S Performance Bank 1 Sensor 2 | ECM | DTC P0133, P0134, P0140, P1133, or P2A00 for the 4.6L (LH2) engine
P2A03 | HO2S Performance Bank 2 Sensor 1 | ECM | DTC P0153,P0154, P0160, P1153, or P2A03 for the 4.6L (LH2) engine
P2A04 | HO2S Performance Bank 2 Sensor 2 | ECM | DTC P0153,P0154, P0160, P1153, or P2A03 for the 4.6L (LH2) engine
U0001 | High Speed CAN Communication Bus | ECM, TCM | DTC U0001
U0002 | Fewer Controllers on Bus Than Programmed | ECM | DTC U0002
U0073 | CAN Bus Circuit Failure | ECM, TCM | DTC U0073
U0100 | Lost Communications with Engine Control Module (ECM) | TCM | DTC U0100-U0299
U0101 | Lost Communications with Transmission Control Module (TCM) | ECM | DTC U0100-U0299
U0121 | Lost Communications with Electronic Brake Control Module (EBCM) | ECM, TCM | DTC U0100-U0299
U140 | Lost Communications with Body Control Module (BCM) | ECM, TCM | DTC U0100-U0299
U0141 | Lost Communications with Instrument Panel Module (IPM) | ECM, TCM | DTC U0100-U0299
U0181 | Lost Communications with Dynamic Headlamp Leveling (DHL) Module | ECM, TCM | DTC U0100-U0299
U0415 | Electronic Brake Control Module (EBCM) Communication Circuit Performance | ECM | DTC U0415
U0423 | Instrument Panel Module (IPM) Communication Circuit Performance | ECM | DTC U0423
U1500 | Inter-device Dedicated Bus | VCIM | DTC U1500
U2100 | Controller Area Network (CAN) Bus Communication | AMP, DDM, DDS, DHL, DPM, DRR, DSCC, EBCM, ESC, HVAC, IPC, IPM, LRDM, PDM, Radio, RCDLR, RIM, RRDM, SCLCM, SDM, TV | DTC U2100
U2103 | Fewer Controllers on Bus Than Programmed | AMP, DDM, DDS, DHL, DPM, DRR, DSCC, EBCM, ESC, HVAC, IPC, IPM, LRDM, PDM, Radio, RCDLR, RIM, RRDM, SCLCM, SDM, TV | DTC U2103
U2105 | Lost Communication with Engine Control Module (ECM) | IPM | DTC U2105-U2199
U2106 | Lost Communications with Transmission Control Module (TCM) | IPM | DTC U2105-U2199
U2108 | Lost Communications with Electronic Brake Control Module (EBCM) | IPM | DTC U2105-U2199
U2112 | Lost Communication With Electronic Suspension Control (ESC) | IPM | DTC U2105-U2199
U2113 | Lost Communication with Sensing and Diagnostic Module (SDM) | IPM | DTC U2105-U2199
U2116 | Lost Communication with Instrument Panel Cluster (IPC) | IPM | DTC U2105-U2199
U2120 | Lost Communication with Dynamic Headlamp Leveling (DHL) Device | IPM | DTC U2105-U2199
U2122 | Lost Communication with Radio | IPM | DTC U2105-U2199
U2124 | Lost Communication with Audio Amplifier (AMP) | IPM | DTC U2105-U2199
U2127 | Lost Communication with HVAC | IPM | DTC U2105-U2199
U2130 | Lost Communication with Driver Door Module (DDM) | IPM | DTC U2105-U2199
U2132 | Lost Communication with Passenger Door Module (PDM) | IPM | DTC U2105-U2199
U2135 | Lost Communication with Rear Integration Module (RIM) | IPM | DTC U2105-U2199
U2162 | Lost Communication with Instrument Panel integration Module (IPM) | RCDLR | DTC U2105-U2199
U2163 | Lost Communication with Left Rear Door Module (LRDM) | IPM | DTC U2105-U2199
U2164 | Lost Communication with Right Rear Door Module (RRDM) | IPM | DTC U2105-U2199
U2165 | Lost Communication with Driver Door Switch (DDS) | IPM | DTC U2105-U2199
U2166 | Lost Communication with Driver Position Module (DPM) | IPM | DTC U2105-U2199
U2167 | Lost Communication with Remote Control Door Lock Receiver (RCDLR) | IPM | DTC U2105-U2199
1049-1050 | PPS System Failure | PPS | DTC 1049-1050
1051 | PPS Start or Preload Failure | PPS | DTC 1051
1052 | PPS Preload Failure Region 1 | PPS | DTC 1052, 1053, 1054, or 1055
1053 | PPS Preload Failure Region 2 | PPS | DTC 1052, 1053, 1054, or 1055
1054 | PPS Preload Failure Region 3 | PPS | DTC 1052, 1053, 1054, or 1055
1055 | PPS Preload Failure Region 4 | PPS | DTC 1052, 1053, 1054, or 1055
1058-1062 | PPS Communication Failure | PPS | DTC 1058-1062
1063 | System Discard | PPS | DTC 1063
2036-2045 | Internal Electronic Performance 2 | PPS | DTC 2036-2045
3011-3035 | Internal Electronic Performance 1 | PPS | DTC 3011-3035