For 1990-2009 cars

#### Special Tools

J 43631 Ball Joint Remover

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the tire and wheel. Refer to Tire and Wheel Removal and Installation.
3. Remove the brake rotor. Refer to Front Brake Rotor Replacement.
4. Using J 43631 remove the wheel stud at the inner most notch.

### Installation Procedure

1. Install the new stud from the back side of the hub.
2. Install flat washers on the wheel stud.

Important: Ensure that the wheel stud is fully seated against the wheel hub flange.

3. With the flat side of a wheel nut against the washers, tighten the wheel nut until the wheel stud head seats against the wheel hub flange.
4. Remove nuts and washers.
5. Install the brake rotor. Refer to Front Brake Rotor Replacement.
6. Install the tire and wheel. Refer to Tire and Wheel Removal and Installation.
7. Lower the vehicle.