For 1990-2009 cars

### Removal Procedure

1. Remove the cross car brace, if necessary. Refer to Cross Vehicle Brace Replacement .
2. Remove the oil fill cap.
3. Disengage the cover/shield from the ball studs by pulling up firmly on the right rear and left front of the engine cover.
4. Remove the engine cover/sight shield.
5. Remove the front compartment sight shield, if necessary. Refer to Front Compartment Sight Shields Replacement .

### Installation Procedure

1. Install the front compartment sight shield, if necessary. Refer to Front Compartment Sight Shields Replacement .
2. Position the engine cover/sight shield over the intake manifold so the grommets are aligned with the ball studs.
3. Press the engine cover/sight shield down firmly near the ball studs in order to install the engine cover/sight shield.
4. Install the oil fill cap.
5. Install the cross car brace, if necessary. Refer to Cross Vehicle Brace Replacement .