For 1990-2009 cars

### Removal Procedure

1. Remove the fuel filler cap.
2. Drain the fuel tank below the level of the fuel filler hose. Refer to Fuel Tank Draining .
3. Remove the bolts securing the fuel filler tube to the body.
4. Remove the right rear wheel. Refer to Tire and Wheel Removal and Installation .
5. Remove the right rear wheelhouse liner. Refer to Rear Wheelhouse Panel Liner Replacement .
6. Remove the fuel filler tube brace bolt.
7. Disconnect the fuel filler hose (1) from the fuel tank.
8. Disconnect the filler vent tube (2) from the evaporative emission (EVAP) hose. Refer to Plastic Collar Quick Connect Fitting Service .
9. Remove the fuel filler tube from the vehicle.

### Installation Procedure

1. Position the fuel filler tube to the vehicle.

Notice: Refer to Component Fastener Tightening Notice in the Preface section.

2. Connect the filler hose (1) to the fuel tank.

Tighten
Tighten the fuel filler tube hose clamp (3) to 3.5 N·m (31 lb in).

3. Connect the filler vent tube (2) to the EVAP hose. Refer to Plastic Collar Quick Connect Fitting Service .

Notice: Refer to Fastener Notice in the Preface section.

4. Install the fuel filler tube brace bolt.

Tighten
Tighten the fuel filler tube brace bolt to 9 N·m (80 lb in).

5. Install the bolts securing the fuel filler tube to the body.

Tighten
Tighten the fuel filler tube bolts to 3.5 N·m (31 lb in).

6. Install the right rear wheelhouse liner. Refer to Rear Wheelhouse Panel Liner Replacement .
7. Install the right rear wheel. Refer to Tire and Wheel Removal and Installation .
8. Add fuel to the fuel tank.
9. Inspect for fuel leaks.
10. Install the fuel filler cap.