For 1990-2009 cars

### Circuit Description

Ground inputs from contacts inside the tilt/telescoping switch. The IPM receives the signal and then sends it via the GMLAN to the memory seat module (MSM). The memory seat module then supplies battery voltage to the tilt motor up or down circuit or the telescope motor in or out circuit depending on which direction of movement is requested.

### DTC Description

This diagnostic procedure supports the following DTC:

DTC B2902 Tilt Telescope 4 Way position switch circuit

(steering column tilt/telescope malfunction)

This vehicle has DTCs which include DTC symptoms. For more information on DTC Symptoms, refer to DTC Symptom Description.

### Conditions for Running the DTC

The IPM is awake, all the voltages are normal.

### Conditions for Setting the DTC

Switch is short to power for more than the calibrated time.

### Action Taken When the DTC Sets

• | It is not available to the tilt/telescope switch input signal, until the DTC is cleared.

• | IPM will turn off the tilt/telescoping function until voltage is normally.

### Conditions for Clearing the MIL/DTC

• | A current DTC will clear when the failed switch input is no longer active.

• | Use a scan tool.

### Diagnostic Aids

An intermittently stuck switch can cause this DTC to set. Refer to Testing for Intermittent Conditions and Poor Connections.

### Test Description

Refer to Schematic and Routing Diagrams in Steering Wheel and Column.