For 1990-2009 cars

Callout | Component Name
--- | ---

#### Rear Side Door Assembly Replacement

1 | Rear Side Door Hinge Lower Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 25 N·m (18 lb ft)
2 | Rear Side Door Hinge Upper Bolt (Qty: 2) Tighten 25 N·m (18 lb ft)
3 | Rear Side Door Assembly Tip Disconnect the rear door wiring harness connector and reconnect when finished with replacement.