For 1990-2009 cars

## Power Seat Adjuster Mechanism Replacement Rear Seat

### Removal Procedure

1. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement
2. Remove rear floor console (only 4.6 premium). Refer to Rear Floor Console Replacement .
3. Remove the fixing bolts between the rear seat adjuster and rear seat back frame.
4. Remove the seat belt anchor bolts.
5. Remove fasteners between the rear seat guide bush and body, take out the seat guide.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the rear seat adjuster, fixing nuts and bolts between rear seat adjuster and body.

Tighten
Tighten the bolt to 60 N·m (44 lb ft).

2. Tighten anchor bolts under seat belt

Tighten
Tighten the bolt to 42 N·m(29 lb ft).

3. Install the fixing bolts between the rear seat adjuster and rear seat back frame.
4. Install the rear floor console. Refer to Rear Floor Console Replacement .
5. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement