For 1990-2009 cars

### Removal Procedure

Warning: Refer to SIR Warning in the Preface section.

1. Disable the SIR system. Refer to SIR Disabling and Enabling.
2. Remove the steering column trim covers. Refer to Steering Column Trim Cover Replacement.
3. Remove the retaining screws from the multifunction switch.
4. Disconnect the multifunction switch electrical connections.
5. Remove the multifunction switch.

### Installation Procedure

1. Connect the multifunction switch electrical connectors.
2. Install the multifunction switch to the steering column.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the retaining screws to the multifunction switch.

Tighten
Tighten the screw to 7 N·m (62 lb in).

4. Install the steering column trim cover. Refer to Steering Column Trim Cover Replacement.
5. Enable the SIR. Refer to SIR Disabling and Enabling.