For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Install a screw jack with a block of wood under the oil pan for support.
3. Remove the lower engine mount retaining nut.
4. Raise the engine using the screw jack until the weight is removed from the mount.
5. Remove the upper engine mount retaining nut.
6. Remove the engine mount from the vehicle.

### Installation Procedure

1. Install the engine mount to the vehicle.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the upper engine mount retaining nut.

Tighten
Tighten the nut to 80 N·m (59 lb ft).

3. Lower the engine using the screw jack until the weight is resting on the mount.
4. Install the engine mount lower retaining nut.

Tighten
Tighten the nut to 80 N·m (59 lb ft).

5. Remove the screw jack and block of wood from under the oil pan.
6. Lower the vehicle.