For 1990-2009 cars

#### Special Tools

• | J 5590 Bearing and Seal Driver

• | J-25254-A Oil Seal Installer

### Left Camshaft Cover

1. Install the NEW left spark plug shield tube seals using the J 5590 (1) and the J-25254-A (2).
2. Install the NEW camshaft cover gasket.
3. Install the oil fill cap.

Caution: Refer to Fastener Caution in the Preface section.

4. Install the fuel injector sight shield cover ballstud.

Tighten
Tighten the fuel injector sight shield cover ball stud to 10 N·m (89 lb in).

Note: The camshaft cover bolt grommet must be installed into the camshaft cover bolt hole before installing the camshaft cover bolt.

Install the NEW left camshaft cover bolt grommets.

### Right Camshaft Cover

1. Install the NEW right spark plug shield tube coil seals using the J 5590 (1) and the J-25254-A (2).
2. Install the NEW right camshaft cover gasket.

Note: The camshaft cover bolt grommet must be installed into the camshaft cover bolt hole before installing the camshaft cover bolt.

3. Install the NEW right camshaft cover bolt grommets.