For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Thoroughly clean the torque converter housing assembly, including threads, with clean solvent.
2. Clean sealing surfaces.
3. Inspect all threaded holes. If necessary, repair any thread damage.

1 | Line Pressure Test Hole Plug
2 | A/Trans Vent Pipe
3 | Trans Fluid Cooler Pipe Fitting Seal Caution: Refer to Seal Reuse Caution in the Preface section. Tip Refer to Transmission Fluid Cooler Pipe Seal Replacement.
4 | Torque Converter Bushing