For 1990-2009 cars

### Removal Procedure

1. Remove the blower and air inlet assembly. Refer to Air Inlet Assembly Replacement.
2. Disconnect the electrical connector from the recirculation actuator.
3. Remove the recirculation actuator screws (1).
4. Remove the recirculation actuator.

### Installation Procedure

1. Install the recirculation actuator.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the recirculation actuator screws (1).

Tighten
Tighten the screws to 1 N·m (9 lb in).

3. Connect the electrical connector to the recirculation actuator.
4. Install the blower and air inlet assembly. Refer to Air Inlet Assembly Replacement.