For 1990-2009 cars

### Removal Procedure

1. Turn the ignition OFF.

Note: Do not disconnect the power steering fluid lines/hoses from the reservoir.

2. Remove the power steering fluid reservoir bolts and reposition the power steering fluid reservoir in order to provide access. Refer to Power Steering Fluid Reservoir Replacement.
3. Remove the camshaft position (CMP) sensor electrical connector.
4. Remove the CMP sensor bolt.
5. Remove the CMP sensor.

### Installation Procedure

1. Install the CMP sensor.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the CMP sensor bolt and tighten to 10 N·m (89 lb in).
3. Install the CMP sensor electrical connector.
4. Install the power steering fluid reservoir. Refer to Power Steering Fluid Reservoir Replacement.