For 1990-2009 cars

### Removal Procedure

1. Disconnect the battery negative cable (2). Refer to Battery Negative Cable Disconnection and Connection.
2. Disconnect the battery positive cable (1) from the battery.
3. Remove the air inlet grille panel. Refer to Air Inlet Grille Panel Replacement.
4. Depress the locking tabs (1) on the side of the battery heat shield.
5. Remove the battery heat shield from the battery.

### Installation Procedure

Important: Ensure the openings in the heat shield are aligned with the battery terminal bosses.

1. Position the battery heat shield downward over the battery.
2. Ensure that the heat shield locking tabs (1) are engaged.
3. Install the air inlet grille panel. Refer to Air Inlet Grille Panel Replacement.

Notice: Refer to Fastener Notice in the Preface section.

4. Connect the battery positive cable (1) to the battery.

Tighten
Tighten the battery positive cable to 17 N·m (13 lb ft).

5. Connect the battery negative cable (2). Refer to Battery Negative Cable Disconnection and Connection.