For 1990-2009 cars

## Radio Rear Speaker Replacement Center

### Removal Procedure

1. Remove the rear shelf trim panel. Refer to Rear Window Shelf Trim Panel Replacement.
2. Remove the nuts securing the center speaker and the right rear speaker (2).
3. Disconnect the electrical connector.
4. Remove the speaker (2).

### Installation Procedure

1. Install the speaker (2).

Notice: Refer to Fastener Notice in the Preface section.

2. Connect the electrical connectors.
3. Install the nuts securing the center speaker and the right rear speaker (2).

Tighten
Tighten the nuts to 9 N·m (80 lb in).

4. Install the rear shelf trim panel. Refer to Rear Window Shelf Trim Panel Replacement.

## Radio Rear Speaker Replacement Left

### Removal Procedure

1. Remove the rear shelf trim panel. Refer to Rear Window Shelf Trim Panel Replacement.
2. Remove the nuts securing the left speaker (1).
3. Disconnect the electrical connector.
4. Remove the speaker (1).

### Installation Procedure

1. Install the speaker (1).
2. Connect the electrical connector.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the nuts securing the left speaker (1).

Tighten
Tighten the nuts to 9 N·m (80 lb in).

4. Install the rear shelf trim panel. Refer to Rear Window Shelf Trim Panel Replacement.