For 1990-2009 cars

### Removal Procedure

Caution: Refer to SIR Caution in the Preface section.

1. Disable the SIR system. Refer to SIR Disabling and Enabling .
2. Remove the steering column trim covers. Refer to Steering Column Trim Covers Replacement .
3. Remove the steering column wiring harness tie straps.
4. Disconnect the electrical connectors (1,3) from the windshield and washer switch.
5. Depress the locking tab (2) on the windshield wiper and washer switch (1) and remove the switch from the steering column.

### Installation Procedure

1. Install the windshield wiper and washer switch (1) to the steering column.
2. Connect the electrical connectors (1,3) on the windshield wiper and washer switch.
3. Route and connect the electrical connector from the windshield wiper and washer switch.
4. Install the wiring harness tie straps.
5. Install the steering column trim covers. Refer to Steering Column Trim Covers Replacement .
6. Enable the SIR system. Refer to SIR Disabling and Enabling .