For 1990-2009 cars

### Removal Procedure

1. Remove rear shelf trim panel. Refer to Rear Window Shelf Trim Panel Replacement.
2. Remove the 7 fasteners securing the carrier assembly to the rear shelf.
3. Disconnect the electrical connector.
4. Remove the rear shelf carrier assembly.

### Installation Procedure

1. Install rear shelf carrier assembly.
2. Connect the electrical connector.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the rear shelf carrier fasteners.

Tighten
Tighten the rear shelf carrier fasteners to 9 N·m (80 lb in).

4. Install the rear shelf trim panel. Refer to Rear Window Shelf Trim Panel Replacement.