For 1990-2009 cars

### Removal Procedure

1. Remove the shifter bezel. Refer to Console Shift Lever Bezel Replacement .
2. Release the tabs (1) on the bottom of the shifter position indicator.
3. Raise the indicator cover in order to access the bulbs mounted on the bottom of the indicator cover.
4. Turn the bulb socket (1) in order to release it from the indicator cover.

### Installation Procedure

1. Locate the bulb socket (1) into the indicator cover.
2. Turn the bulb socket (1) in order to secure it to the indicator cover.
3. Lower the indicator cover onto the shifter assembly.
4. Push the cover in order to secure the tabs (1) on the bottom of the shifter position indicator.
5. Install the shifter bezel. Refer to Console Shift Lever Bezel Replacement .