For 1990-2009 cars

### Removal Procedure

1. Remove the air inlet grille panel. Refer to Air Inlet Grille Panel Replacement .
2. With two hands release the tabs on each side of the access cover.
3. Lift up the filter access cover (1).
4. Remove the filter (1) from the filter housing.
5. Gently pry out on the filter housing to separate the housing from the sheet metal.
6. Remove the passenger air filter housing (1).

### Installation Procedure

1. Install the passenger air filter housing (1).
2. Press the passenger air filter housing until all clips engage into the sheet metal.
3. Ensure that there is a good seal between the passenger air filter housing and the sheet metal.
4. Install the filter (1) into the filter housing.
5. Install the filter access cover (1).
6. Install the air inlet grille panel. Refer to Air Inlet Grille Panel Replacement .