For 1990-2009 cars

## Rear SeatAudio Control Replacement Base

### Removal Procedure

1. Remove the trim panel of rear seat entertainment console panel.
2. Remove the nuts securing the rear seat entertainment console panel.
3. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.
2. Install the nuts securing the rear seat entertainment console panel.
3. Install the trim panel of rear seat entertainment console panel.

## Rear SeatAudio Control Replacement Luxury

### Removal Procedure

1. Remove the rear console bezel from the rear console. Refer to Rear Floor Console Rear Trim Upper Panel Replacement .
2. Remove the bolts securing the audio model.
3. Remove the audio module from the rear console. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.
2. Install the audio module and secure the screws.
3. Install the rear console bezel. Refer to Rear Floor Console Rear Trim Upper Panel Replacement .