For 1990-2009 cars

## Sunshade Replacement Windshield Sunshade

### Removal Procedure

1. Detach the sunshade (1) from the sunshade rod retainer clip.
2. Remove the windshield pillar molding. Refer to Windshield Pillar Garnish Molding Replacement.
3. Remove the fasteners from the outboard bezel (2).

Note: The sunshade bezel is secured to the roof by means of a two piece plastic retainer and metal integral clip.

4. The plastic retainer will fall out of the headliner (3) when the three fasteners are removed from the bezel.

Caution: Use care when removing or installing the headliner. Excessive bending will damage the headliner.

5. Carefully reach inside the headliner until the electrical connector (1) is exposed.
6. Disconnect the electrical connector.
7. Remove the sunshade from the vehicle.

### Installation Procedure

1. Position the sunshade to the headliner.
2. Push the electrical connector and the wiring through the hole in the headliner.
3. Connect the electrical connector (1).
4. Position the plastic retainer (2) over the top of the electrical harness.
5. Align the fasteners to the holes in the sunshade metal integral clip (2).

Caution: Refer to Fastener Caution in the Preface section.

Note: Do not pinch the wiring (3) when you install the fasteners.

6. Install the fasteners that secure the bezel (2) to the headliner.

Tighten
Tighten the fasteners to 2 N·m (18 lb in).

7. Install the windshield pillar garnish molding. Refer to Windshield Pillar Garnish Molding Replacement.
8. Secure the sunshade to the sunshade rod retainer.

## Sunshade Replacement Door Sunshade

### Removal Procedure

1. Remove the rear side door trim panel. Refer to Side Door Sill Nameplate Replacement.
2. Remove the fastening screws of the rear window sunshade from the back of the rear side door trim panel.

### Installation Procedure

1. Install the rear window sunshade to the rear door trim panel.
2. Install the mounting screws of the door sunshade.
3. Install the rear side door trim panel. Refer to Side Door Sill Nameplate Replacement.

## Sunshade Replacement Sail Sunshade

### Removal Procedure

1. Remove the rear side door trim panel. Refer to Rear Side Door Trim Panel Replacement.
2. Remove the mounting screws of the sunshade from the door. Loosen the bottom end of the sunshade.
3. Pull downward the sail sunshade. Loosen the locking tab inserted into the window frame at the top end of the sunshade.
4. Remove the sunshade.

### Installation Procedure

1. Insert the top end of the locking tab into the sail sunshade.
2. Install the mounting screws at the bottom end of the sail sunshade.
3. Install the rear side door trim panel. Refer to Rear Side Door Trim Panel Replacement Sill Trim Plate Replacement, Rear Side Door .