For 1990-2009 cars

Callout | Component Name
--- | ---

#### Rear Bumper Fascia Replacement

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the rear wheelhouse liner panels. Refer to Rear Wheelhouse Panel Liner Replacement .

1 | Rear Bumper Fascia Screw Notice: Refer to Fastener Notice in the Preface section. Tip The screws are in the wheel opening. Tighten
3 N·m (27 lb in)

2 | Compartment Sill Trim Plate Assembly
3 | Rear Bumper Fascia Screw (Qty: 4) Tighten 6 N·m (53 lb in)
4 | Rear Bumper Fascia Retainer (Qty: 3) Tip Remove the retainer with inclined cutter, replace with new retainer while installing.
5 | Rear Bumper Fascia Assembly Tighten 6 N·m (5 lb in)

#### Rear Bumper Impact Bar Assembly Replacement

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the rear wheelhouse liner panels. Refer to Rear Wheelhouse Panel Liner Replacement .

1 | Rear Bumper Fascia Screw Tip The screws are in the wheel opening. Tighten 3 N·m (27 lb in)
2 | Compartment Sill Trim Plate Assembly
3 | Rear Bumper Fascia Screw (Qty: 4) Tighten 6 N·m (5 lb in)
4 | Rear Bumper Fascia Retainer (Qty: 3) Tip Remove the retainer with inclined cutter, replace with new retainer while installing.
5 | Rear Bumper Fascia Assembly Tighten 6 N·m (53 lb in)
6 | Rear Bumper Impact Bar Bolt (Qty: 8) Tighten 25 N·m (18 lb ft)
7 | Rear Bumper Impact Bar Assembly

#### Rear Bumper Energy Absorber Assembly

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the rear wheelhouse liner panels. Refer to Rear Wheelhouse Panel Liner Replacement .

1 | Rear Bumper Fascia Screw Tip The screws are in the wheel opening. Tighten 3 N·m (27 lb in)
2 | Compartment Sill Trim Plate Assembly
3 | Rear Bumper Fascia Screw (Qty: 4) Tighten 6 N·m (53 lb in)
4 | Rear Bumper Fascia Retainer (Qty: 3) Tip Remove the retainer with inclined cutter, replace with new retainer while installing.
5 | Rear Bumper Fascia Assembly Tighten 6 N·m (53 lb in)
6 | Rear Bumper Impact Bar Bolt (Qty: 8) Tighten 25 N·m (18 lb ft)
7 | Rear Bumper Impact Bar Assembly
8 | Rear Bumper Energy Absorber Bolt (Qty: 2) Tighten 25 N·m (18 lb ft)
9 | Rear Bumper Energy Absorber Nut (Qty: 4) Tighten 25 N·m (18 lb ft)
10 | Rear Bumper Energy Absorber Assembly

#### Rear Bumper Fascia Bracket Replacement

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the rear wheelhouse liner panels. Refer to Rear Wheelhouse Panel Liner Replacement .

1 | Rear Bumper Fascia Screw Tip The screws are in the wheel opening. Tighten 3 N·m (27 lb in)
2 | Compartment Sill Trim Plate Assembly
3 | Rear Bumper Fascia Bolt (Qty: 4) Tighten 6 N·m (53 lb in)
4 | Rear Bumper Fascia Retainer (Qty: 3) Tip Remove the retainer with inclined cutter, replace with new retainer while installing.
5 | Rear Bumper Fascia Assembly Tighten 6 N·m (53 lb in)
11 | Rear Bumper Fascia Bracket Screw (Qty: 10) Tighten 3 N·m (27 lb in)
12 | Rear Bumper Fascia Bracket (Qty: 2)

#### Rear Bumper Fascia Insert Replacement

13 | Rear Bumper Fascia Insert Locator (Qty: 2)
14 | Rear Bumper Fascia Insert