For 1990-2009 cars

### Removal Procedure

1. Remove the generator and water pump drive belt. Refer to Water Pump and Generator Belt Replacement.
2. Loosen the drive belt tensioner bolt.
3. Remove the drive belt tensioner and bolt from the engine.

### Installation Procedure

1. Position the drive belt tensioner and bolt to the engine as an assembly.
2. Ensure that the alignment pin on the rear of the tensioner assembly is aligned with the locating hole on the engine.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the drive belt tensioner bolt.

Tighten
Tighten the drive belt tensioner bolt to 50 N·m (37 lb ft).

4. Install the generator and water pump drive belt. Refer to Water Pump and Generator Belt Replacement.