For 1990-2009 cars

### Removal Procedure

1. Remove center pillar garnish molding. Refer to Center Pillar Garnish Molding Replacement.
2. Insert a pointed tool into the hole (1) in order to release the seat belt from the seat.
3. Remove the bolts securing the seat belt assembly to the vehicle.

### Installation Procedure

1. Install the bolts securing the seat belt assembly to the vehicle.

Tighten
Tighten the seat belt fastening bolt to 40 N·m(29 lb ft).

2. Install center pillar garnish molding. Refer to Center Pillar Garnish Molding Replacement .
3. Reinstall the seat belt to the seat (1).