For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front seats. Refer to Driver or Passenger Seat Replacement .

1 | Front Floor Console Refer to Front Floor Console Replacement .
2 | Auxiliary Air Outlet Duct Screw Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (17 lb in)
3 | Passenger Side Auxiliary Floor Air Duct Tip Reposition the carpet to access the rear floor air ducts.
4 | Driver Side Auxiliary Floor Air Duct Tip Use blunt trim tool to release the tabs to separate the auxiliary floor ducts.
5 | Retainer Push Pin (Qty: 1) Tip There is 1 push-in retainer per floor - rear air outlet duct.
6 | Floor Rear Air Outlet