For 1990-2009 cars

Callout | Component Name
--- | ---

#### Windshield Solvent Container Level Sensor Replacement

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the air deflector assembly. Refer to Front Air Deflector Replacement.

1 | Windshield Washer Fluid Level Switch Seal
2 | Windshield Washer Fluid Level Switch Tip

1. Bleed the washer fluid, re-fill after replacement.
2. Disconnect the electrical connectors and re-connect after replacement.
3. Use two flat-bladed tools to pry outward the washer fluid level sensor switch (1) from the washer fluid reservoir.
4. Use the same inward pressure to press the fluid level sensor into the seals.