For 1990-2009 cars

1. Install the engine control module (ECM) bracket.

Notice: Refer to Fastener Notice in the Preface section.

2. Loosely install the ECM bracket bolts.

Tighten

1. Tighten the side ECM bracket bolts to 10 N·m(89 lb in).
2. Tighten the front ECM bracket bolts to 23 N·m(17 lb ft).

3. Install the ECM module to the ECM bracket.
4. Install the ECM module bolts.

Tighten
Tighten the ECM module bolts to 10 N·m (89 lb in).

5. Install the engine wiring harness to the engine.
6. Connect the engine wiring harness to the right camshaft position sensors.
7. Install the engine wiring harness ground bolt to the ECM bracket.

Tighten
Tighten the engine wiring harness ground bolt to 10 N·m (89 lb in).

8. Install the engine wiring harness ground bolt to the side of the right cylinder head.

Tighten
Tighten the engine wiring harness ground bolt to 10 N·m (89 lb in).

9. Connect the engine wiring harness to the evaporative emission (EVAP) solenoid.
10. Connect the engine wiring harness to the right oxygen sensor harness.
11. Connect the engine wiring harness to the right knock sensor.
12. Connect the engine wiring harness to the generator.
13. Connect the engine wiring harness to the fuel injector harness.
14. Connect the engine wiring harness to the right ignition coils.
15. Connect the engine wiring harness to the right camshaft position actuator valves.
16. Connect the engine wiring harness to the front of the right camshaft cover.
17. Position the ECM ground harness ring terminal to ECM lug and install the ECM ground harness ring terminal screw.

Tighten
Tighten the ECM ground harness ring terminal screw to 4.5 N·m (40 lb in).

18. Connect the engine wiring harness to the left side of the throttle body/intake manifold.
19. Connect the engine wiring harness to the top of the right camshaft cover.
20. Install the engine wiring harness bracket bolt to the top of the ECM bracket.

Tighten
Tighten the engine wiring harness bracket bolt to 10 N·m (89 lb in).

21. Install the engine wiring harness bracket bolt to the side of the ECM bracket.

Tighten
Tighten the engine wiring harness bracket bolt to 23 N·m (17 lb ft).

22. Connect the engine wiring harness to the crankshaft position sensor.
23. Install the engine wiring harness bracket bolt.

Tighten
Tighten the engine wiring harness bracket bolt to 50 N·m (37 lb ft).

24. Connect the engine wiring harness to the ECM module.
25. Install the battery cable ground.
26. Install the battery cable ground bolt to the rear of the left cylinder head.

Tighten
Tighten the battery cable ground bolt to 50 N·m (37 lb ft).

27. Connect the battery cable to the generator.
28. Install the battery cable/generator nut to the generator.

Tighten
Tighten the battery cable/generator nut to 13 N·m (115 lb in).

29. Connect the battery cable harness to the right side of the engine.
30. Connect the engine wiring harness to the barometric pressure (BARO) sensor.
31. Connect the engine wiring harness to the left camshaft position sensors.
32. Install the engine wiring harness ground bolt to the left cylinder head.

Tighten
Tighten the engine wiring harness ground bolt to 10 N·m (89 lb in).

33. Connect the engine wiring harness to the engine coolant temperature (ECT) sensor.
34. Connect the engine wiring harness to the throttle body connector.
35. Connect the engine wiring harness to the starter motor solenoid.
36. Connect the engine wiring harness to the left oxygen sensor harness.
37. Connect the engine wiring harness to the oil pressure sender.
38. Connect the engine wiring harness to the communicator valve.
39. Connect the engine wiring harness to the left knock sensor.
40. Connect the engine wiring harness to the left ignition coils.
41. Connect the engine wiring harness to the left camshaft position actuator valves.
42. Connect the engine wiring harness to the A/C compressor.
43. Connect the engine wiring harness to the front of the left camshaft cover.
44. Connect the engine wiring harness to the top of the left camshaft cover.
45. Install the engine wiring harness bracket bolts to the lower left side of the engine.

Tighten
Tighten the engine wiring harness bracket bolts to 10 N·m (89 lb in).

46. Install the engine wiring harness bracket bolt to the lower right side of the engine.

Tighten
Tighten the engine wiring harness bracket bolt to 10 N·m (89 lb in).

47. Install the engine wiring harness bracket stud to the lower right side of the engine.

Tighten
Tighten the engine wiring harness bracket stud to 22 N·m (16 lb ft).

48. Connect the battery cable harness to the starter motor.
49. Install the radiator outlet pipe.
50. Install the radiator outlet pipe bolt to the thermostat housing and the generator bracket.

Tighten
Tighten the radiator outlet pipe bolt to the thermostat housing and the generator bracket to 23 N·m (17 lb in).

51. Install the radiator outlet pipe bolt to the rear of the right cylinder head.

Tighten
Tighten the radiator outlet pipe bolt to 50 N·m (27 lb ft).

52. Install the right exhaust manifold lower insulator.
53. Install the right exhaust manifold lower insulator nuts.

Tighten
Tighten the right exhaust manifold lower insulator nuts to 10 N·m (89 lb in).

54. Install the intake manifold insulator.
55. Install the intake manifold insulator nut.

Tighten
Tighten the intake manifold insulator nut to 10 N·m (89 lb in).