For 1990-2009 cars

## Power Steering Fluid Reservoir Replacement LH2

### Removal Procedure

1. Remove the air cleaner intake duct. Refer to Air Cleaner Outlet Duct Replacement.
2. Remove the front air deflector. Refer to Front Air Deflector Replacement.
3. Place a drain pan under the vehicle.
4. Disconnect the power steering cooler hose from the power steering reservoir.
5. Disconnect the power steering reservoir outlet hose from the power steering reservoir.
6. Remove the power steering reservoir retaining nuts.
7. Remove the power steering reservoir from the vehicle.

### Installation Procedure

1. Install the power steering reservoir to the vehicle.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the power steering reservoir retaining nuts.

Tighten
Tighten the nuts to 9 N·m (80 lb in).

3. Connect the power steering reservoir outlet hose to the power steering reservoir.
4. Connect the power steering cooler hose to the power steering reservoir.
5. Remove the drain pan from under the vehicle.
6. Install the air filter intake duct. Refer to Air Cleaner Outlet Duct Replacement.
7. Bleed the power steering system. Refer to Power Steering System Bleeding.
8. Install the front air deflector. Refer to Front Air Deflector Replacement.

## Power Steering Fluid Reservoir Replacement LY7

### Removal Procedure

1. Remove the fuel injector sight shield. Refer to Fuel Injector Sight Shield Replacement.
2. Remove the front air deflector. Refer to Front Air Deflector Replacement.
3. Place a drain pan under the vehicle.
4. Disconnect the power steering cooler hose from the power steering reservoir.
5. Disconnect the power steering reservoir outlet hose from the power steering reservoir.
6. Remove the power steering reservoir retaining bolts.
7. Remove the power steering reservoir from the vehicle.

### Installation Procedure

1. Install the power steering reservoir to the vehicle.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the power steering reservoir retaining bolts.

Tighten
Tighten the bolts to 9 N·m (80 lb in).

3. Connect the power steering reservoir outlet hose to the power steering reservoir.
4. Connect the power steering cooler hose to the power steering reservoir.
5. Remove the drain pan from under the vehicle.
6. Bleed the power steering system. Refer to Power Steering System Bleeding.
7. Install the front air deflector. Refer to Front Air Deflector Replacement.
8. Install the fuel injection sight shield. Refer to Fuel Injector Sight Shield Replacement.