For 1990-2009 cars

### Removal Procedure

1. Remove the front floor console extension trim panel. Refer to Front Floor Console Extension Panel Replacement .
2. Remove the bolts securing the rear of cupholder to the front floor console extension trim panel.
3. Remove the cupholder from the front floor console.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the front floor console cupholder.

Tighten
Tighten the screws to 2 N·m (18 lb in).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the bolts securing the cupholder to the front floor console extension trim panel.

Tighten
Tighten the screws to 2 N·m (18 lb in).

3. Install the front floor console extension trim panel. Refer to Front Floor Console Extension Panel Replacement .