For 1990-2009 cars

## Power Seat Switch Replacement Rear Seat

### Removal Procedure

1. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement.
2. Pry open the rear seat adjuster switch assembly.
3. Disconnect the electrical connector.
4. Pry open the rear seat adjuster switch button.
5. Pry open the buckle on the switch trim panel with a flat bladed tool, take out switches.

### Installation Procedure

1. Install the switch onto the switch trim panel.
2. Install rear seat adjuster switch button.
3. Connect the electrical connectors.
4. Install the rear seat adjuster switch assembly onto the rear seat cushion.
5. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement.

## Power Seat Switch Replacement Front Seat

Callout | Component Name
--- | ---

#### Preliminary Procedures

Remove the front seat adjuster switch trim panel assembly. Refer to Front Seat Trim Panel Replacement.

1 | Front Seat Adjuster Switch Button Tip Pull the front seat adjuster switch button out from the trim panel.
2 | Front Seat Bezel Adjuster Switch Tip Use a flat-bladed tool to pry off the switch trim panel buckle and pull the seat adjuster switch out.
3 | Front Seat Lumbar Control Switch Tip Pull out the switch button from trim panel, use a flat-bladed tool to pry off the switch trim panel buckle and pull out the seat lumbar control switch.