For 1990-2009 cars

### Removal Procedure

1. Release the retaining clips using a blunt trim tool to remove center console panel. Refer to Front Floor Console Replacement .
2. Remove auxiliary HVAC control module retaining screws.
3. Remove auxiliary HVAC control module.
4. Disconnect auxiliary HVAC control module electrical connectors, remove the module.

### Installation Procedure

1. Connect the auxiliary HVAC control module electrical connectors.
2. Install auxiliary HVAC control module.

Notice: Refer to Fastener Notice in the Preface section.

3. Install auxiliary HVAC control module retaining screws.

Tighten
Tighten the screw to 2 N·m (80 lb in).

4. Install the center console panel. Refer to Front Floor Console Replacement .