For 1990-2009 cars

### Removal Procedure

Important: The wiper blades need to be cycled to the mid-wipe position to prevent the wiper arms contacting the rear edge of the hood.

1. Cycle the wiper blades of the mid-wipe position on the glass.
2. Push in the button of the wiper blade clip and remove the wiper blade from the inside radius of the wiper arm.
3. Take out the wiper arm through the opening in the wiper blade.

### Installation Procedure

1. Insert the hook of the wiper arm through the opening in the wiper blade.
2. Position the wiper blade pivot in the inside radius of the wiper arm hook.
3. Pull the wiper blade pivot into the wiper arm hook until the pivot locks into the hook.
4. Ensure the blade is locked onto the wiper arm.
5. Return the wiper blades to the park position.
6. Operate the wiper and inspect for normal operation.