For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel retainer. Refer to Instrument Panel Carrier Replacement .
2. Press in on the tab to release the defroster duct (1) from the HVAC module.
3. Remove the defroster duct (1).

### Installation Procedure

1. Remove the defroster duct (1).
2. Press down on the defroster duct (1) until you hear the tabs engage.
3. Install the instrument panel retainer. Refer to Instrument Panel Carrier Replacement .