For 1990-2009 cars

Callout | Component Name
--- | ---
High Mounted Stop Lamp Assembly Replacement Preliminary Procedure

1. Open the rear compartment lid.
2. Remove the rear compartment lid inner panel trim assembly. Refer to Rear Compartment Trim, Lid, Latch, Strut, Hinge Replacement in Body Rear End.

1 | High Mounted Stop Lamp Nuts (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 4 N·m (35 lb in)
2 | High Mounted Stop Lamp Electrical Connector
3 | High Mounted Stop Lamp Assembly Tip The high mounted stop lamp is LED and there are no replaceable bulbs. The lamp assembly must be replaced as an assembly.