For 1990-2009 cars

Callout | Component Name
--- | ---
Backup Lamp Assembly Replacement Preliminary Procedure

1. Open the rear compartment lid.
2. Remove the rear compartment lid inner panel trim assembly. Refer to Rear Compartment Trim, Lid, Latch, Strut, Hinge Replacement in Body Rear End.

1 | Backup Lamp Nuts (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 6 N·m (53 lb in)
2 | Backup Lamp Electrical Connector
3 | Backup Lamp Assembly Tip If only replacing the bulb, turn bulb socket assembly and pull out of the lamp assembly. This can be done from the inside of the rear compartment lid without removing the lamp from the vehicle.